{"text_format":"3","workbook":"xlsx","n_sheets":24,"sheets":["表-08 分部分项工程和单价措施项目清单与计价表【一体化泵","表-11 总价措施项目清单与计价汇总表【一体化泵站】","表-13 规费、税金项目计价表【一体化泵站】","表-14 主要材料价格表【一体化泵站】","表-08 分部分项工程和单价措施项目清单与计价表【景观看台】","表-11 总价措施项目清单与计价汇总表【景观看台】","表-13 规费、税金项目计价表【景观看台】","表-14 主要材料价格表【景观看台】","表-08 分部分项工程和单价措施项目清单与计价表【景观工程】","表-11 总价措施项目清单与计价汇总表【景观工程】","表-13 规费、税金项目计价表【景观工程】","表-14 主要材料价格表【景观工程】","表-08 分部分项工程和单价措施项目清单与计价表【园林绿化】","表-11 总价措施项目清单与计价汇总表【园林绿化】","表-13 规费、税金项目计价表【园林绿化】","表-14 主要材料价格表【园林绿化】","表-08 分部分项工程和单价措施项目清单与计价表【电气工程】","表-11 总价措施项目清单与计价汇总表【电气工程】","表-13 规费、税金项目计价表【电气工程】","表-14 主要材料价格表【电气工程】","表-08 分部分项工程和单价措施项目清单与计价表【排水工程】","表-11 总价措施项目清单与计价汇总表【排水工程】","表-13 规费、税金项目计价表【排水工程】","表-14 主要材料价格表【排水工程】"],"read":"whole","date_system":"1900"}

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表【一体化泵","index":0,"n_rows":76,"n_cols":11,"rows_kept":76,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,10],[3,7,4,7],[3,8,4,9],[5,3,5,4],[5,8,5,9],[6,3,6,4],[6,8,6,9],[7,3,7,4],[7,8,7,9],[8,3,8,4],[8,8,8,9],[9,3,9,4],[9,8,9,9],[10,3,10,4],[10,8,10,9],[11,3,11,4],[11,8,11,9],[12,3,12,4],[12,8,12,9],[13,0,13,7],[13,8,13,9],[14,0,14,10],[15,0,15,3],[15,4,15,8],[15,9,15,10],[16,0,16,10],[17,0,17,3],[17,4,17,8],[17,9,17,10],[18,0,20,0],[18,1,20,1],[18,2,20,2],[18,3,20,4],[18,5,20,5],[18,6,20,6],[18,7,18,10],[19,7,20,7],[19,8,20,9],[21,3,21,4],[21,8,21,9],[22,3,22,4],[22,8,22,9],[23,3,23,4],[23,8,23,9],[24,3,24,4],[24,8,24,9],[25,3,25,4],[25,8,25,9],[26,3,26,4],[26,8,26,9],[27,0,27,7],[27,8,27,9],[28,0,28,10],[29,0,29,3],[29,4,29,8],[29,9,29,10],[30,0,30,10],[31,0,31,3],[31,4,31,8],[31,9,31,10],[32,0,34,0],[32,1,34,1],[32,2,34,2],[32,3,34,4],[32,5,34,5],[32,6,34,6],[32,7,32,10],[33,7,34,7],[33,8,34,9],[35,3,35,4],[35,8,35,9],[36,3,36,4],[36,8,36,9],[37,3,37,4],[37,8,37,9],[38,3,38,4],[38,8,38,9],[39,3,39,4],[39,8,39,9],[40,3,40,4],[40,8,40,9],[41,3,41,4],[41,8,41,9],[42,3,42,4],[42,8,42,9],[43,3,43,4],[43,8,43,9],[44,3,44,4],[44,8,44,9],[45,0,45,7],[45,8,45,9],[46,0,46,10],[47,0,47,3],[47,4,47,8],[47,9,47,10],[48,0,48,10],[49,0,49,3],[49,4,49,8],[49,9,49,10],[50,0,52,0],[50,1,52,1],[50,2,52,2],[50,3,52,4],[50,5,52,5],[50,6,52,6],[50,7,50,10],[51,7,52,7],[51,8,52,9],[53,3,53,4],[53,8,53,9],[54,3,54,4],[54,8,54,9],[55,3,55,4],[55,8,55,9],[56,3,56,4],[56,8,56,9],[57,3,57,4],[57,8,57,9],[58,3,58,4],[58,8,58,9],[59,3,59,4],[59,8,59,9],[60,3,60,4],[60,8,60,9],[61,3,61,4],[61,8,61,9],[62,3,62,4],[62,8,62,9],[63,3,63,4],[63,8,63,9],[64,3,64,4],[64,8,64,9],[65,3,65,4],[65,8,65,9],[66,3,66,4],[66,8,66,9],[67,3,67,4],[67,8,67,9],[68,3,68,4],[68,8,68,9],[69,3,69,4],[69,8,69,9],[70,3,70,4],[70,8,70,9],[71,3,71,4],[71,8,71,9],[72,0,72,7],[72,8,72,9],[73,0,73,7],[73,8,73,9],[74,0,74,10],[75,0,75,3],[75,4,75,8],[75,9,75,10]]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：一体化泵站",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 1 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"土石方工程"]
[1,"010101004001","挖基坑土方","1.名称:挖装一般土方\n2.土壤类别:一、二类土\n3.挖土深度:详见图纸\n4.其他:详见图纸设计及相关规范要求",null,"m3","408.84"]
[2,"010103001001","回填方","1.回填部位:基础（挡墙内侧与设备之间）\n2.土质要求:1:8水泥土回填\n3.回填方式:夯填\n4.取土运距:自行考虑\n5.其他:详见图纸设计及相关规范要求",null,"m3","58.51"]
[3,"010103001002","回填方","1.回填部位:挡土墙外侧到筏板边\n2.土质要求:素土回填\n3.回填方式:夯填\n4.取土运距:自行考虑\n5.其他:详见图纸设计及相关规范要求",null,"m3","73.25"]
[4,"040103002001","余方弃置","1.余方弃置\n2.弃土运距:1KM",null,"m3","335.59"]
[null,null,"分部小计"]
[null,null,"混凝土及钢筋混凝土工程"]
[1,"010507007001","其他构件","1.部位:泵站筒体安装完成后，底部灌浆\n2.混凝土种类:素混凝土\n3.混凝土强度等级:C30\n4.其他说明:详见图纸设计及相关规范要求",null,"m3","12.49"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：一体化泵站",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 2 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[2,"010201017001","褥垫层","1.名称:褥垫层\n2.种类:碎石垫层\n3其他说明:详见图纸设计及相关规范要求",null,"m3","13.94"]
[3,"010501001001","垫层","1.名称:混凝土垫层\n2.混凝土强度等级:C15\n3.商品砼泵送方式:泵车\n4.其他说明:详见图纸设计及相关规范要求",null,"m3","12.15"]
[4,"010501004001","满堂基础","1.名称:筏板基础\n2.混凝土种类:商品混凝土\n3.混凝土强度等级:C30 P6\n4.商品砼泵送方式:泵车\n5.其他说明:详见图纸设计及相关规范要求",null,"m3","27.22"]
[5,"010504004001","挡土墙","1.名称:挡土墙\n2.混凝土种类:商品混凝土\n3.混凝土强度等级:C30 \n4.商品砼泵送方式:泵车\n5.其他说明:详见图纸设计及相关规范要求",null,"m3","30.6"]
[6,"010515001001","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400E以内 直径 12\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.761"]
[7,"010515001002","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400E以内 直径 14\n2.其他说明:详见图纸设计及相关规范要求",null,"t","4.738"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：一体化泵站",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 3 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[8,"010515001003","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400E以内 直径 18\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.315"]
[9,"010515001004","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400E以内 直径 20\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.236"]
[10,"010515001005","现浇构件钢筋","1.钢筋种类、规格:箍筋 带肋钢筋HPB300以内 直径 ≤10mm\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.058"]
[null,null,"分部小计"]
[null,null,"其他装饰工程"]
[1,"080701005001","钢管预埋","1.挡土墙内预埋钢管\n2.其他说明:详见图纸设计及相关规范要求",null,"m","0.6"]
[2,"010606011001","止水钢板","1.部位:墙体水平施工缝应留在距底板、顶板500mm以上处，当墙体有孔洞时,施工缝距孔洞边缘不宜小于300mm。施工缝应加设-400x3镀锌钢板\n止水。",null,"m","20.4"]
[null,null,"分部小计"]
[null,null,"措施项目"]
[1,"011702001001","垫层","1.基础类型:垫层\n2.其他说明:详见图纸设计及相关规范要求",null,"m2","8.64"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：一体化泵站",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 4 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[2,"011702001002","基础","1.基础类型:满堂基础\n2.其他说明:详见图纸设计及相关规范要求",null,"m2","20.4"]
[3,"041102017001","挡土墙模板","1.基础类型:挡土墙模板\n2.其他说明:详见图纸设计及相关规范要求",null,"m2","102"]
[4,"011701002001","外脚手架","1.3.6m以外混凝土墙脚手架\n2.其他说明:详见图纸设计及相关规范要求",null,"m2","108"]
[5,"011703001001","垂直运输","1.地下一层\n2.其他说明：详见图纸设计及相关规范说明",null,"m2","29.16"]
[6,"011705001001","大型机械设备进出场及安拆","1.挖掘机1台\n2.其他说明:详见图纸设计及相关规范要求",null,"台·次","1"]
{"$rows_empty":14}
["本页小计"]
["合  计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]

{"sheet":"表-11 总价措施项目清单与计价汇总表【一体化泵站】","index":1,"n_rows":34,"n_cols":11,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,7],[1,8,1,10],[2,3,2,4],[2,7,2,8],[3,3,3,4],[3,7,3,8],[4,3,4,4],[4,7,4,8],[5,3,5,4],[5,7,5,8],[6,3,6,4],[6,7,6,8],[7,3,7,4],[7,7,7,8],[8,3,8,4],[8,7,8,8],[9,3,9,4],[9,7,9,8],[10,3,10,4],[10,7,10,8],[11,3,11,4],[11,7,11,8],[12,3,12,4],[12,7,12,8],[13,3,13,4],[13,7,13,8],[14,3,14,4],[14,7,14,8],[15,3,15,4],[15,7,15,8],[16,3,16,4],[16,7,16,8],[17,3,17,4],[17,7,17,8],[18,3,18,4],[18,7,18,8],[19,3,19,4],[19,7,19,8],[20,3,20,4],[20,7,20,8],[21,3,21,4],[21,7,21,8],[22,3,22,4],[22,7,22,8],[23,3,23,4],[23,7,23,8],[24,3,24,4],[24,7,24,8],[25,3,25,4],[25,7,25,8],[26,3,26,4],[26,7,26,8],[27,3,27,4],[27,7,27,8],[28,3,28,4],[28,7,28,8],[29,3,29,4],[29,7,29,8],[30,0,30,5],[30,7,30,8],[31,0,31,3],[31,4,31,7],[31,8,31,10],[32,0,32,10],[33,0,33,3],[33,4,33,7],[33,8,33,10]]}
["总价措施项目清单与计价表"]
["工程名称：一体化泵站",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":3},"第 1 页 共 1 页"]
["序号","项目编码","项 目 名 称","计 算 基 础",null,"费率(%)","金 额(元)","调整费\n率(%)",null,"调整后金额\n(元)","备 注"]
["1","011707001001","安全文明施工费","分部分项安全文明施工费+单价措施安全文明施工费"]
["2","01","其他措施费（费率类）"]
["2.1","011707002001","夜间施工增加费","分部分项其他措施费+单价措施其他措施费"]
["2.2","011707004001","二次搬运费","分部分项其他措施费+单价措施其他措施费"]
["2.3","011707005001","冬雨季施工增加费","分部分项其他措施费+单价措施其他措施费"]
["3","02","其他（费率类）"]
{"$rows_empty":21}
["合  计"]
["编制人（造价人员）：",{"$nulls":3},"复核人（造价工程师）："]
["注：1.“计算基础”中安全文明施工费可为“定额基价”、“定额人工费”或“定额人工费+定额机械费”，其他项目可为“定额人工费”或“定额人工费+定额机械费”。\n    2.按施工方案计算的措施费，若无“计算基础”和“费率”的数值，也可只填“金额”数值，但应在备注栏说明施工方案出处或计算方法。"]
[{"$nulls":8},"表-11"]

{"sheet":"表-13 规费、税金项目计价表【一体化泵站】","index":2,"n_rows":37,"n_cols":8,"rows_kept":37,"merged":[[0,0,0,7],[1,0,1,2],[1,3,1,5],[1,6,1,7],[2,2,2,3],[2,5,2,6],[3,2,3,3],[3,5,3,6],[4,2,4,3],[4,5,4,6],[5,2,5,3],[5,5,5,6],[6,2,6,3],[6,5,6,6],[7,2,7,3],[7,5,7,6],[8,2,8,3],[8,5,8,6],[9,2,9,3],[9,5,9,6],[10,2,10,3],[10,5,10,6],[11,2,11,3],[11,5,11,6],[12,2,12,3],[12,5,12,6],[13,2,13,3],[13,5,13,6],[14,2,14,3],[14,5,14,6],[15,2,15,3],[15,5,15,6],[16,2,16,3],[16,5,16,6],[17,2,17,3],[17,5,17,6],[18,2,18,3],[18,5,18,6],[19,2,19,3],[19,5,19,6],[20,2,20,3],[20,5,20,6],[21,2,21,3],[21,5,21,6],[22,2,22,3],[22,5,22,6],[23,2,23,3],[23,5,23,6],[24,2,24,3],[24,5,24,6],[25,2,25,3],[25,5,25,6],[26,2,26,3],[26,5,26,6],[27,2,27,3],[27,5,27,6],[28,2,28,3],[28,5,28,6],[29,2,29,3],[29,5,29,6],[30,2,30,3],[30,5,30,6],[31,2,31,3],[31,5,31,6],[32,2,32,3],[32,5,32,6],[33,2,33,3],[33,5,33,6],[34,0,34,4],[34,5,34,6],[35,0,35,2],[35,3,35,7],[36,0,36,2],[36,3,36,5],[36,6,36,7]]}
["规费、税金项目计价表"]
["工程名称：一体化泵站",null,null,"标段：襄城县塔湾坑水生态治理及应急排涝项目",null,null,"第 1 页 共 1 页"]
["序号","项 目 名 称","计 算 基 础",null,"计算基数","计算费率\n(%)",null,"金 额(元)"]
["1","规费","定额规费+工程排污费+其他"]
["1.1","定额规费","分部分项规费+单价措施规费"]
["1.2","工程排污费"]
["1.3","其他"]
["2","增值税","不含税工程造价合计"]
{"$rows_empty":26}
["合  计"]
[" 编制人（造价人员）：",null,null,"复核人（造价工程师）："]
[{"$nulls":6},"表—13"]

{"sheet":"表-14 主要材料价格表【一体化泵站】","index":3,"n_rows":7,"n_cols":10,"rows_kept":7,"merged":[[0,0,0,9],[1,0,1,1],[1,2,1,7],[1,8,1,9],[2,1,2,2],[2,7,2,8],[3,1,3,2],[3,7,3,8],[4,1,4,2],[4,7,4,8],[5,1,5,2],[5,7,5,8],[6,1,6,2],[6,7,6,8],[7,1,7,2],[7,7,7,8],[8,1,8,2],[8,7,8,8],[9,1,9,2],[9,7,9,8],[10,1,10,2],[10,7,10,8],[11,1,11,2],[11,7,11,8],[12,1,12,2],[12,7,12,8],[13,1,13,2],[13,7,13,8],[14,1,14,2],[14,7,14,8],[15,1,15,2],[15,7,15,8],[16,1,16,2],[16,7,16,8],[17,1,17,2],[17,7,17,8],[18,1,18,2],[18,7,18,8],[19,1,19,2],[19,7,19,8],[20,1,20,2],[20,7,20,8],[21,1,21,2],[21,7,21,8],[22,1,22,2],[22,7,22,8],[23,1,23,2],[23,7,23,8],[24,1,24,2],[24,7,24,8],[25,1,25,2],[25,7,25,8],[26,1,26,2],[26,7,26,8],[27,1,27,2],[27,7,27,8],[28,1,28,2],[28,7,28,8],[29,1,29,2],[29,7,29,8],[30,1,30,2],[30,7,30,8],[31,1,31,2],[31,7,31,8],[32,1,32,2],[32,7,32,8],[33,1,33,2],[33,7,33,8],[34,1,34,2],[34,7,34,8],[35,1,35,2],[35,7,35,8],[36,1,36,2],[36,7,36,8]]}
["主要材料价格表"]
["工程名称：",null,"一体化泵站",{"$nulls":5},"第 1 页 共 1 页"]
["序号","材料编码",null,"材料名称","规格、型号\n等特殊要求","单位","数 量","单 价",null,"合 价"]
[1,"04010129@1",null,"水泥","42.5","t"]
[2,"04050173",null,"碎石","综合","m3"]
[3,"80210555",null,"预拌混凝土","C15","m3"]
[4,"80210561",null,"预拌混凝土","C30","m3"]

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表【景观看台】","index":4,"n_rows":52,"n_cols":11,"rows_kept":52,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,10],[3,7,4,7],[3,8,4,9],[5,3,5,4],[5,8,5,9],[6,3,6,4],[6,8,6,9],[7,3,7,4],[7,8,7,9],[8,3,8,4],[8,8,8,9],[9,3,9,4],[9,8,9,9],[10,3,10,4],[10,8,10,9],[11,3,11,4],[11,8,11,9],[12,3,12,4],[12,8,12,9],[13,0,13,7],[13,8,13,9],[14,0,14,10],[15,0,15,3],[15,4,15,8],[15,9,15,10],[16,0,16,10],[17,0,17,3],[17,4,17,8],[17,9,17,10],[18,0,20,0],[18,1,20,1],[18,2,20,2],[18,3,20,4],[18,5,20,5],[18,6,20,6],[18,7,18,10],[19,7,20,7],[19,8,20,9],[21,3,21,4],[21,8,21,9],[22,3,22,4],[22,8,22,9],[23,3,23,4],[23,8,23,9],[24,3,24,4],[24,8,24,9],[25,3,25,4],[25,8,25,9],[26,3,26,4],[26,8,26,9],[27,0,27,7],[27,8,27,9],[28,0,28,10],[29,0,29,3],[29,4,29,8],[29,9,29,10],[30,0,30,10],[31,0,31,3],[31,4,31,8],[31,9,31,10],[32,0,34,0],[32,1,34,1],[32,2,34,2],[32,3,34,4],[32,5,34,5],[32,6,34,6],[32,7,32,10],[33,7,34,7],[33,8,34,9],[35,3,35,4],[35,8,35,9],[36,3,36,4],[36,8,36,9],[37,3,37,4],[37,8,37,9],[38,3,38,4],[38,8,38,9],[39,3,39,4],[39,8,39,9],[40,3,40,4],[40,8,40,9],[41,3,41,4],[41,8,41,9],[42,3,42,4],[42,8,42,9],[43,3,43,4],[43,8,43,9],[44,3,44,4],[44,8,44,9],[45,3,45,4],[45,8,45,9],[46,3,46,4],[46,8,46,9],[47,3,47,4],[47,8,47,9],[48,0,48,7],[48,8,48,9],[49,0,49,7],[49,8,49,9],[50,0,50,10],[51,0,51,3],[51,4,51,8],[51,9,51,10]]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观看台",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 1 页 共 3 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"土石方工程"]
[1,"010101004002","挖基坑土方","1.名称:挖装一般土方\n2.土壤类别:一、二类土\n3.挖土深度:详见图纸\n4.其他:详见图纸设计及相关规范要求",null,"m3","507.3"]
[2,"010103001003","回填方","1.回填部位:基础\n2.土质要求:素土回填\n3.回填方式:夯填\n4.取土运距:自行考虑\n5.其他:详见图纸设计及相关规范要求",null,"m3","484.27"]
[3,"040103002002","余方弃置","1.余方弃置\n2.弃土运距:1KM",null,"m3","23.03"]
[null,null,"分部小计"]
[null,null,"混凝土及钢筋混凝土工程"]
[1,"010501001002","垫层","1.名称:混凝土垫层\n2.混凝土强度等级:C15\n3.商品砼泵送方式:泵车\n4.其他说明:详见图纸设计及相关规范要求",null,"m3","3.15"]
[2,"010501003001","独立基础","1.名称:独立基础\n2.混凝土种类:商品混凝土\n3.混凝土强度等级:C30\n4.商品砼泵送方式:泵车\n5.其他说明:详见图纸设计及相关规范要求",null,"m3","12.31"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观看台",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 2 页 共 3 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[3,"010509002001","圆形柱","1.混凝土种类:商品混凝土\n2.混凝土强度等级:C30\n3.商品砼泵送方式:泵车\n4.其他说明:详见图纸设计及相关规范要求",null,"m3","1.88"]
[4,"010503002001","矩形梁","1.混凝土种类:商品混凝土\n2.混凝土强度等级:C30\n3.商品砼泵送方式:泵车\n4.其他说明:详见图纸设计及相关规范要求",null,"m3","4.33"]
[5,"010505003001","平板","1.混凝土种类:商品混凝土\n2.混凝土强度等级:C30\n3.商品砼泵送方式:泵车\n4.其他说明:详见图纸设计及相关规范要求",null,"m3","8.04"]
[6,"010515001006","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400E以内 直径 ≤10mm\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.756"]
[7,"010515001007","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400E以内 直径 14mm\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.75"]
[8,"010515001008","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400E以内 直径 ≤16\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.533"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观看台",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 3 页 共 3 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[9,"010515001009","现浇构件钢筋","1.钢筋种类、规格:箍筋 带肋钢筋HPB300以内 直径 ≤10mm\n2.其他说明:详见图纸设计及相关规范要求",null,"t","0.359"]
[10,"010516003001","机械连接","1.连接方式:直螺纹连接\n2.规格:16以内\n3.其他说明:详见图纸设计及相关规范要求",null,"个","18"]
[null,null,"分部小计"]
[null,null,"措施项目"]
[1,"011702001003","垫层","1.基础类型:垫层\n2.其他说明:详见图纸设计及相关规范要求",null,"m2","8.4"]
[2,"011702001004","基础","1.基础类型:独立基础\n2.其他说明:详见图纸设计及相关规范要求",null,"m2","32.76"]
[3,"011702004001","圆形柱","1.部位:圆柱\n2.层高:3.6m\n3.其他说明:详见图纸设计及相关规范要求",null,"m2","21.2"]
[4,"011702006001","矩形梁","1.部位:矩形梁\n2.层高:3.6m\n3.其他说明:详见图纸设计及相关规范要求",null,"m2","53.07"]
[5,"011702016001","平板","1.部位:平板\n2.层高:3.6m\n3.其他说明:详见图纸设计及相关规范要求",null,"m2","62.27"]
[]
[]
[]
[]
["本页小计"]
["合  计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]

{"sheet":"表-11 总价措施项目清单与计价汇总表【景观看台】","index":5,"n_rows":34,"n_cols":11,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,7],[1,8,1,10],[2,3,2,4],[2,7,2,8],[3,3,3,4],[3,7,3,8],[4,3,4,4],[4,7,4,8],[5,3,5,4],[5,7,5,8],[6,3,6,4],[6,7,6,8],[7,3,7,4],[7,7,7,8],[8,3,8,4],[8,7,8,8],[9,3,9,4],[9,7,9,8],[10,3,10,4],[10,7,10,8],[11,3,11,4],[11,7,11,8],[12,3,12,4],[12,7,12,8],[13,3,13,4],[13,7,13,8],[14,3,14,4],[14,7,14,8],[15,3,15,4],[15,7,15,8],[16,3,16,4],[16,7,16,8],[17,3,17,4],[17,7,17,8],[18,3,18,4],[18,7,18,8],[19,3,19,4],[19,7,19,8],[20,3,20,4],[20,7,20,8],[21,3,21,4],[21,7,21,8],[22,3,22,4],[22,7,22,8],[23,3,23,4],[23,7,23,8],[24,3,24,4],[24,7,24,8],[25,3,25,4],[25,7,25,8],[26,3,26,4],[26,7,26,8],[27,3,27,4],[27,7,27,8],[28,3,28,4],[28,7,28,8],[29,3,29,4],[29,7,29,8],[30,0,30,5],[30,7,30,8],[31,0,31,3],[31,4,31,7],[31,8,31,10],[32,0,32,10],[33,0,33,3],[33,4,33,7],[33,8,33,10]]}
["总价措施项目清单与计价表"]
["工程名称：景观看台",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":3},"第 1 页 共 1 页"]
["序号","项目编码","项 目 名 称","计 算 基 础",null,"费率(%)","金 额(元)","调整费\n率(%)",null,"调整后金额\n(元)","备 注"]
["1","011707001001","安全文明施工费","分部分项安全文明施工费+单价措施安全文明施工费"]
["2","01","其他措施费（费率类）"]
["2.1","011707002001","夜间施工增加费","分部分项其他措施费+单价措施其他措施费"]
["2.2","011707004001","二次搬运费","分部分项其他措施费+单价措施其他措施费"]
["2.3","011707005001","冬雨季施工增加费","分部分项其他措施费+单价措施其他措施费"]
["3","02","其他（费率类）"]
{"$rows_empty":21}
["合  计"]
["编制人（造价人员）：",{"$nulls":3},"复核人（造价工程师）："]
["注：1.“计算基础”中安全文明施工费可为“定额基价”、“定额人工费”或“定额人工费+定额机械费”，其他项目可为“定额人工费”或“定额人工费+定额机械费”。\n    2.按施工方案计算的措施费，若无“计算基础”和“费率”的数值，也可只填“金额”数值，但应在备注栏说明施工方案出处或计算方法。"]
[{"$nulls":8},"表-11"]

{"sheet":"表-13 规费、税金项目计价表【景观看台】","index":6,"n_rows":37,"n_cols":8,"rows_kept":37,"merged":[[0,0,0,7],[1,0,1,2],[1,3,1,5],[1,6,1,7],[2,2,2,3],[2,5,2,6],[3,2,3,3],[3,5,3,6],[4,2,4,3],[4,5,4,6],[5,2,5,3],[5,5,5,6],[6,2,6,3],[6,5,6,6],[7,2,7,3],[7,5,7,6],[8,2,8,3],[8,5,8,6],[9,2,9,3],[9,5,9,6],[10,2,10,3],[10,5,10,6],[11,2,11,3],[11,5,11,6],[12,2,12,3],[12,5,12,6],[13,2,13,3],[13,5,13,6],[14,2,14,3],[14,5,14,6],[15,2,15,3],[15,5,15,6],[16,2,16,3],[16,5,16,6],[17,2,17,3],[17,5,17,6],[18,2,18,3],[18,5,18,6],[19,2,19,3],[19,5,19,6],[20,2,20,3],[20,5,20,6],[21,2,21,3],[21,5,21,6],[22,2,22,3],[22,5,22,6],[23,2,23,3],[23,5,23,6],[24,2,24,3],[24,5,24,6],[25,2,25,3],[25,5,25,6],[26,2,26,3],[26,5,26,6],[27,2,27,3],[27,5,27,6],[28,2,28,3],[28,5,28,6],[29,2,29,3],[29,5,29,6],[30,2,30,3],[30,5,30,6],[31,2,31,3],[31,5,31,6],[32,2,32,3],[32,5,32,6],[33,2,33,3],[33,5,33,6],[34,0,34,4],[34,5,34,6],[35,0,35,2],[35,3,35,7],[36,0,36,2],[36,3,36,5],[36,6,36,7]]}
["规费、税金项目计价表"]
["工程名称：景观看台",null,null,"标段：襄城县塔湾坑水生态治理及应急排涝项目",null,null,"第 1 页 共 1 页"]
["序号","项 目 名 称","计 算 基 础",null,"计算基数","计算费率\n(%)",null,"金 额(元)"]
["1","规费","定额规费+工程排污费+其他"]
["1.1","定额规费","分部分项规费+单价措施规费"]
["1.2","工程排污费"]
["1.3","其他"]
["2","增值税","不含税工程造价合计"]
{"$rows_empty":26}
["合  计"]
[" 编制人（造价人员）：",null,null,"复核人（造价工程师）："]
[{"$nulls":6},"表—13"]

{"sheet":"表-14 主要材料价格表【景观看台】","index":7,"n_rows":5,"n_cols":10,"rows_kept":5,"merged":[[0,0,0,9],[1,0,1,1],[1,2,1,7],[1,8,1,9],[2,1,2,2],[2,7,2,8],[3,1,3,2],[3,7,3,8],[4,1,4,2],[4,7,4,8],[5,1,5,2],[5,7,5,8],[6,1,6,2],[6,7,6,8],[7,1,7,2],[7,7,7,8],[8,1,8,2],[8,7,8,8],[9,1,9,2],[9,7,9,8],[10,1,10,2],[10,7,10,8],[11,1,11,2],[11,7,11,8],[12,1,12,2],[12,7,12,8],[13,1,13,2],[13,7,13,8],[14,1,14,2],[14,7,14,8],[15,1,15,2],[15,7,15,8],[16,1,16,2],[16,7,16,8],[17,1,17,2],[17,7,17,8],[18,1,18,2],[18,7,18,8],[19,1,19,2],[19,7,19,8],[20,1,20,2],[20,7,20,8],[21,1,21,2],[21,7,21,8],[22,1,22,2],[22,7,22,8],[23,1,23,2],[23,7,23,8],[24,1,24,2],[24,7,24,8],[25,1,25,2],[25,7,25,8],[26,1,26,2],[26,7,26,8],[27,1,27,2],[27,7,27,8],[28,1,28,2],[28,7,28,8],[29,1,29,2],[29,7,29,8],[30,1,30,2],[30,7,30,8],[31,1,31,2],[31,7,31,8],[32,1,32,2],[32,7,32,8],[33,1,33,2],[33,7,33,8],[34,1,34,2],[34,7,34,8],[35,1,35,2],[35,7,35,8],[36,1,36,2],[36,7,36,8]]}
["主要材料价格表"]
["工程名称：",null,"景观看台",{"$nulls":5},"第 1 页 共 1 页"]
["序号","材料编码",null,"材料名称","规格、型号\n等特殊要求","单位","数 量","单 价",null,"合 价"]
[1,"80210555",null,"预拌混凝土","C15","m3"]
[2,"80210561",null,"预拌混凝土","C30","m3"]

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表【景观工程】","index":8,"n_rows":94,"n_cols":11,"rows_kept":94,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,10],[3,7,4,7],[3,8,4,9],[5,3,5,4],[5,8,5,9],[6,3,6,4],[6,8,6,9],[7,3,7,4],[7,8,7,9],[8,0,8,7],[8,8,8,9],[9,0,9,10],[10,0,10,3],[10,4,10,8],[10,9,10,10],[11,0,11,10],[12,0,12,3],[12,4,12,8],[12,9,12,10],[13,0,15,0],[13,1,15,1],[13,2,15,2],[13,3,15,4],[13,5,15,5],[13,6,15,6],[13,7,13,10],[14,7,15,7],[14,8,15,9],[16,3,16,4],[16,8,16,9],[17,3,17,4],[17,8,17,9],[18,3,18,4],[18,8,18,9],[19,3,19,4],[19,8,19,9],[20,3,20,4],[20,8,20,9],[21,0,21,7],[21,8,21,9],[22,0,22,10],[23,0,23,3],[23,4,23,8],[23,9,23,10],[24,0,24,10],[25,0,25,3],[25,4,25,8],[25,9,25,10],[26,0,28,0],[26,1,28,1],[26,2,28,2],[26,3,28,4],[26,5,28,5],[26,6,28,6],[26,7,26,10],[27,7,28,7],[27,8,28,9],[29,3,29,4],[29,8,29,9],[30,3,30,4],[30,8,30,9],[31,3,31,4],[31,8,31,9],[32,3,32,4],[32,8,32,9],[33,3,33,4],[33,8,33,9],[34,3,34,4],[34,8,34,9],[35,3,35,4],[35,8,35,9],[36,0,36,7],[36,8,36,9],[37,0,37,10],[38,0,38,3],[38,4,38,8],[38,9,38,10],[39,0,39,10],[40,0,40,3],[40,4,40,8],[40,9,40,10],[41,0,43,0],[41,1,43,1],[41,2,43,2],[41,3,43,4],[41,5,43,5],[41,6,43,6],[41,7,41,10],[42,7,43,7],[42,8,43,9],[44,3,44,4],[44,8,44,9],[45,3,45,4],[45,8,45,9],[46,3,46,4],[46,8,46,9],[47,3,47,4],[47,8,47,9],[48,3,48,4],[48,8,48,9],[49,3,49,4],[49,8,49,9],[50,3,50,4],[50,8,50,9],[51,3,51,4],[51,8,51,9],[52,3,52,4],[52,8,52,9],[53,3,53,4],[53,8,53,9],[54,0,54,7],[54,8,54,9],[55,0,55,10],[56,0,56,3],[56,4,56,8],[56,9,56,10],[57,0,57,10],[58,0,58,3],[58,4,58,8],[58,9,58,10],[59,0,61,0],[59,1,61,1],[59,2,61,2],[59,3,61,4],[59,5,61,5],[59,6,61,6],[59,7,59,10],[60,7,61,7],[60,8,61,9],[62,3,62,4],[62,8,62,9],[63,3,63,4],[63,8,63,9],[64,3,64,4],[64,8,64,9],[65,3,65,4],[65,8,65,9],[66,3,66,4],[66,8,66,9],[67,3,67,4],[67,8,67,9],[68,3,68,4],[68,8,68,9],[69,0,69,7],[69,8,69,9],[70,0,70,10],[71,0,71,3],[71,4,71,8],[71,9,71,10],[72,0,72,10],[73,0,73,3],[73,4,73,8],[73,9,73,10],[74,0,76,0],[74,1,76,1],[74,2,76,2],[74,3,76,4],[74,5,76,5],[74,6,76,6],[74,7,74,10],[75,7,76,7],[75,8,76,9],[77,3,77,4],[77,8,77,9],[78,3,78,4],[78,8,78,9],[79,3,79,4],[79,8,79,9],[80,3,80,4],[80,8,80,9],[81,3,81,4],[81,8,81,9],[82,3,82,4],[82,8,82,9],[83,3,83,4],[83,8,83,9],[84,3,84,4],[84,8,84,9],[85,3,85,4],[85,8,85,9],[86,3,86,4],[86,8,86,9],[87,3,87,4],[87,8,87,9],[88,3,88,4],[88,8,88,9],[89,3,89,4],[89,8,89,9],[90,0,90,7],[90,8,90,9],[91,0,91,7],[91,8,91,9],[92,0,92,10],[93,0,93,3],[93,4,93,8],[93,9,93,10]]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 1 页 共 6 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"生态护坡"]
[1,"040305005001","护坡（上部斜坡部分）","1.120厚C25空心六角块混凝土构件(清水混凝土面，内种植草皮)\n2.30厚1:6干硬性水泥砂浆\n3.150厚C25砼,内加A6@100X100防裂钢丝网片\n4.50厚中粗砂垫层\n5.两布一膜,单层土工布型号为200g/平米,膜为天然钠基膨润土防水毯\n6.50厚中粗砂垫层\n7.素土夯实,夯实系数≥94%\n8.其他说明:详见图纸设计及相关规范要求",null,"m2","459.22"]
[2,"040305005002","护坡（下部斜坡部分）","1.120厚C25实心六角块混凝土构件(清水混凝土面)\n2.30厚1:6干硬性水泥砂浆\n3.150厚C25砼,内加A6@100X100防裂钢丝网片\n4.100厚中粗砂垫层\n5.两布一膜,单层土工布型号为200g/平米,膜为天然钠基膨润土防水毯\n6.100厚中粗砂垫层\n7.素土夯实,夯实系数≥94%\n8.其他说明:详见图纸设计及相关规范要求",null,"m2","503.81"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 2 页 共 6 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[3,"040305005003","护坡（中间平台部分）","1.280厚C25砼,内加A6@100X100防裂钢丝网片\n2.50厚中粗砂垫层\n3.两布一膜,单层土工布型号为200g/平米,膜为天然钠基膨润土防水毯\n4.50厚中粗砂垫层\n5.素土夯实,夯实系数≥94%\n6.其他说明:详见图纸设计及相关规范要求",null,"m2","221.41"]
[4,"040305005004","支墩（上下部与平台交界处）","1.C25砼\n2.50厚中粗砂垫层\n3.两布一膜,单层土工布型号为200g/平米,膜为天然钠基膨润土防水毯\n4.50厚中粗砂垫层\n5.素土夯实,夯实系数≥94%\n6.其他说明:详见图纸设计及相关规范要求",null,"m2","163.87"]
[5,"040601006001","池底","1.300厚砂质土\n2.两布一膜,单层土工布型号为200g/平米,膜为天然钠基膨润土防水毯\n3.50厚中粗砂找平层\n4.素土夯实,夯实系数≥94%\n5.其他说明:详见图纸设计及相关规范要求",null,"m2","1544.94"]
[null,null,"分部小计"]
[null,null,"环形道路硬化（彩色沥青）"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 3 页 共 6 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[1,"040203006001","沥青混凝土","图集15J012-1 路20/D6\n1.30厚改性细粒式彩色沥青石屑面层\n2.100厚碎石\n3.150厚3:7灰土\n4.素土夯实\n5.其他说明:详见图纸设计及相关规范要求",null,"m2","287.08"]
[2,"040204004001","安砌侧(平、缘）石","1.600*150*150厚芝麻灰花岗岩侧石\n2.30厚1:3水泥砂浆\n3.C20混凝土护靠\n4.110厚C20混凝土\n5.素土夯实\n6.其他说明:详见图纸设计及相关规范要求",null,"m","262.37"]
[null,null,"分部小计"]
[null,null,"活动场地硬化（透水砖铺装）"]
[1,"040204002001","人行道块料铺设","1.300*600mm生态仿石陶瓷颗粒透水砖\n2.30厚1：3水泥砂浆\n3.100厚C25素混凝土\n4.200厚6%水泥石粉渣垫层\n5.素土夯实\n6.其他说明:详见图纸设计及相关规范要求",null,"m2","385.48"]
[2,"040204004002","安砌侧(平、缘）石","1.600*150*150厚芝麻灰花岗岩侧石\n2.30厚1:3水泥砂浆\n3.C20混凝土护靠\n4.110厚C20混凝土\n5.素土夯实\n6.其他说明:详见图纸设计及相关规范要求",null,"m","71.65"]
[null,null,"分部小计"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 4 页 共 6 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"坑塘护栏（花岗岩材质）"]
[1,"040309002001","石质栏杆","1.花岗岩护栏\n2.深色花岗岩收边\n3.预埋2φ14-L=400，1:2膨胀水泥砂浆\n4.C25砼\n5.50厚中粗砂垫层\n6.两布一膜，单层土工布型号200g/m2，膜为天然纳基膨润土防水毯\n7.50厚中粗砂垫层\n8.素土夯实，夯实系数≥94%\n9.其他说明:详见图纸设计及相关规范要求",null,"m","251.04"]
[null,null,"分部小计"]
[null,null,"条石凳"]
[1,"020202006001","条形石座凳","1.素土夯实\n2.110厚C20垫层\n3.30厚1:3水泥砂浆\n4.400mm高光面花岗岩芝麻白整石\n5.其他说明:详见图纸设计及相关规范要求",null,"m","4.8"]
[2,"050305007001","成品花岗岩桌凳","1.样式详图15/08\n2.其他说明:详见图纸设计及相关规范要求",null,"套","3"]
[null,null,"分部小计"]
[null,null,"树池"]
[1,"040204007001","树池砌筑","1.素土夯实\n2.50厚φ25~35颗粒白色卵石\n3.内侧种植葱兰\n4.其他说明:详见图纸设计及相关规范要求",null,"个","9"]
[null,null,"分部小计"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 5 页 共 6 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"其他"]
[1,"011104002001","竹、木（复合）地板","1.95X45塑木地板\n2.55X55防腐木龙骨@500\n3.详见图纸设计及相关规范要求",null,"m2","60.45"]
[2,"050307009001","文化信息牌","1.文化信息牌\n2.不锈钢材质,高2m,宽1.8m,厚0.08m,不锈钢材质,由专业厂家深化制作、安装\n3.其他说明:详见图纸设计及相关规范要求",null,"套","1"]
[3,"050307017001","垃圾收集设备","1.垃圾收集设备\n2.不锈钢材质,成品,具体样式由业主选定,高1.8m,宽0.8m,长2m\n3.其他说明:详见图纸设计及相关规范要求",null,"个","1"]
[4,"050307009002","救生圈","1.救生圈\n2.其他说明:详见图纸设计及相关规范要求",null,"套","4"]
[5,"050307009003","水岸警示标识（大）","1.水岸警示标识\n2.不锈钢材质,高1.5m,宽0.6m,厚0.06m,不锈钢材质,由专业厂家深化制作、安装\n3.其他说明:详见图纸设计及相关规范要求",null,"套","4"]
[6,"050307009004","水岸警示标识（小）","1.水岸警示标识\n2.不锈钢材质,单个高15cm,宽40cm,由专业厂家深化制作、安装\n3.其他说明:详见图纸设计及相关规范要求",null,"套","4"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：景观工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 6 页 共 6 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[7,"050307009005","草地警示标识","1.草地警示标识\n2.不锈钢材质,高40cm,宽30cm,由专业厂家深化制作、安装\n3.其他说明:详见图纸设计及相关规范要求",null,"套","5"]
[8,"050307014001","木制花箱","1.木制花箱\n2.成品木材质,长80cm,高60cm,宽40cm,内种植海桐篱,由专业厂家安装\n3.其他说明:详见图纸设计及相关规范要求",null,"个","10"]
[9,"050307014002","健身器材","1.健身器材5个\n2.成品不锈钢材质\n3.其他说明:详见图纸设计及相关规范要求",null,"套","1"]
[null,null,"分部小计"]
[null,null,"措施项目"]
[1,"041106001001","大型机械设备进出场及安拆","1.进出场费 压路机\n2.进出场费 沥青混凝土摊铺机\n3.进出场费 履带式 挖掘机\n4.进出场费 履带式 推土机\n5.其他说明:详见相关设计图纸、要求及规范",null,"项","1"]
{"$rows_empty":7}
["本页小计"]
["合  计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]

{"sheet":"表-11 总价措施项目清单与计价汇总表【景观工程】","index":9,"n_rows":34,"n_cols":11,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,7],[1,8,1,10],[2,3,2,4],[2,7,2,8],[3,3,3,4],[3,7,3,8],[4,3,4,4],[4,7,4,8],[5,3,5,4],[5,7,5,8],[6,3,6,4],[6,7,6,8],[7,3,7,4],[7,7,7,8],[8,3,8,4],[8,7,8,8],[9,3,9,4],[9,7,9,8],[10,3,10,4],[10,7,10,8],[11,3,11,4],[11,7,11,8],[12,3,12,4],[12,7,12,8],[13,3,13,4],[13,7,13,8],[14,3,14,4],[14,7,14,8],[15,3,15,4],[15,7,15,8],[16,3,16,4],[16,7,16,8],[17,3,17,4],[17,7,17,8],[18,3,18,4],[18,7,18,8],[19,3,19,4],[19,7,19,8],[20,3,20,4],[20,7,20,8],[21,3,21,4],[21,7,21,8],[22,3,22,4],[22,7,22,8],[23,3,23,4],[23,7,23,8],[24,3,24,4],[24,7,24,8],[25,3,25,4],[25,7,25,8],[26,3,26,4],[26,7,26,8],[27,3,27,4],[27,7,27,8],[28,3,28,4],[28,7,28,8],[29,3,29,4],[29,7,29,8],[30,0,30,5],[30,7,30,8],[31,0,31,3],[31,4,31,7],[31,8,31,10],[32,0,32,10],[33,0,33,3],[33,4,33,7],[33,8,33,10]]}
["总价措施项目清单与计价表"]
["工程名称：景观工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":3},"第 1 页 共 1 页"]
["序号","项目编码","项 目 名 称","计 算 基 础",null,"费率(%)","金 额(元)","调整费\n率(%)",null,"调整后金额\n(元)","备 注"]
["1","011707001001","安全文明施工费","分部分项安全文明施工费+单价措施安全文明施工费"]
["2","01","其他措施费（费率类）"]
["2.1","011707002001","夜间施工增加费","分部分项其他措施费+单价措施其他措施费"]
["2.2","011707004001","二次搬运费","分部分项其他措施费+单价措施其他措施费"]
["2.3","011707005001","冬雨季施工增加费","分部分项其他措施费+单价措施其他措施费"]
["3","02","其他（费率类）"]
{"$rows_empty":21}
["合  计"]
["编制人（造价人员）：",{"$nulls":3},"复核人（造价工程师）："]
["注：1.“计算基础”中安全文明施工费可为“定额基价”、“定额人工费”或“定额人工费+定额机械费”，其他项目可为“定额人工费”或“定额人工费+定额机械费”。\n    2.按施工方案计算的措施费，若无“计算基础”和“费率”的数值，也可只填“金额”数值，但应在备注栏说明施工方案出处或计算方法。"]
[{"$nulls":8},"表-11"]

{"sheet":"表-13 规费、税金项目计价表【景观工程】","index":10,"n_rows":37,"n_cols":8,"rows_kept":37,"merged":[[0,0,0,7],[1,0,1,2],[1,3,1,5],[1,6,1,7],[2,2,2,3],[2,5,2,6],[3,2,3,3],[3,5,3,6],[4,2,4,3],[4,5,4,6],[5,2,5,3],[5,5,5,6],[6,2,6,3],[6,5,6,6],[7,2,7,3],[7,5,7,6],[8,2,8,3],[8,5,8,6],[9,2,9,3],[9,5,9,6],[10,2,10,3],[10,5,10,6],[11,2,11,3],[11,5,11,6],[12,2,12,3],[12,5,12,6],[13,2,13,3],[13,5,13,6],[14,2,14,3],[14,5,14,6],[15,2,15,3],[15,5,15,6],[16,2,16,3],[16,5,16,6],[17,2,17,3],[17,5,17,6],[18,2,18,3],[18,5,18,6],[19,2,19,3],[19,5,19,6],[20,2,20,3],[20,5,20,6],[21,2,21,3],[21,5,21,6],[22,2,22,3],[22,5,22,6],[23,2,23,3],[23,5,23,6],[24,2,24,3],[24,5,24,6],[25,2,25,3],[25,5,25,6],[26,2,26,3],[26,5,26,6],[27,2,27,3],[27,5,27,6],[28,2,28,3],[28,5,28,6],[29,2,29,3],[29,5,29,6],[30,2,30,3],[30,5,30,6],[31,2,31,3],[31,5,31,6],[32,2,32,3],[32,5,32,6],[33,2,33,3],[33,5,33,6],[34,0,34,4],[34,5,34,6],[35,0,35,2],[35,3,35,7],[36,0,36,2],[36,3,36,5],[36,6,36,7]]}
["规费、税金项目计价表"]
["工程名称：景观工程",null,null,"标段：襄城县塔湾坑水生态治理及应急排涝项目",null,null,"第 1 页 共 1 页"]
["序号","项 目 名 称","计 算 基 础",null,"计算基数","计算费率\n(%)",null,"金 额(元)"]
["1","规费","定额规费+工程排污费+其他"]
["1.1","定额规费","分部分项规费+单价措施规费"]
["1.2","工程排污费"]
["1.3","其他"]
["2","增值税","不含税工程造价合计"]
{"$rows_empty":26}
["合  计"]
[" 编制人（造价人员）：",null,null,"复核人（造价工程师）："]
[{"$nulls":6},"表—13"]

{"sheet":"表-14 主要材料价格表【景观工程】","index":11,"n_rows":9,"n_cols":10,"rows_kept":9,"merged":[[0,0,0,9],[1,0,1,1],[1,2,1,7],[1,8,1,9],[2,1,2,2],[2,7,2,8],[3,1,3,2],[3,7,3,8],[4,1,4,2],[4,7,4,8],[5,1,5,2],[5,7,5,8],[6,1,6,2],[6,7,6,8],[7,1,7,2],[7,7,7,8],[8,1,8,2],[8,7,8,8],[9,1,9,2],[9,7,9,8],[10,1,10,2],[10,7,10,8],[11,1,11,2],[11,7,11,8],[12,1,12,2],[12,7,12,8],[13,1,13,2],[13,7,13,8],[14,1,14,2],[14,7,14,8],[15,1,15,2],[15,7,15,8],[16,1,16,2],[16,7,16,8],[17,1,17,2],[17,7,17,8],[18,1,18,2],[18,7,18,8],[19,1,19,2],[19,7,19,8],[20,1,20,2],[20,7,20,8],[21,1,21,2],[21,7,21,8],[22,1,22,2],[22,7,22,8],[23,1,23,2],[23,7,23,8],[24,1,24,2],[24,7,24,8],[25,1,25,2],[25,7,25,8],[26,1,26,2],[26,7,26,8],[27,1,27,2],[27,7,27,8],[28,1,28,2],[28,7,28,8],[29,1,29,2],[29,7,29,8],[30,1,30,2],[30,7,30,8],[31,1,31,2],[31,7,31,8],[32,1,32,2],[32,7,32,8],[33,1,33,2],[33,7,33,8],[34,1,34,2],[34,7,34,8],[35,1,35,2],[35,7,35,8],[36,1,36,2],[36,7,36,8]]}
["主要材料价格表"]
["工程名称：",null,"景观工程",{"$nulls":5},"第 1 页 共 1 页"]
["序号","材料编码",null,"材料名称","规格、型号\n等特殊要求","单位","数 量","单 价",null,"合 价"]
[1,"04030139@2",null,"砂子","中粗砂","m3"]
[2,"04050173",null,"碎石","综合","m3"]
[3,"36070306@1",null,"芝麻灰花岗岩侧石","600*150*150","m"]
[4,"80210557",null,"预拌混凝土","C20","m3"]
[5,"80210559",null,"预拌混凝土","C25","m3"]
[6,"补充主材001@1",null,"30厚沥青石屑面层","改性细粒式","m3"]

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表【园林绿化】","index":12,"n_rows":75,"n_cols":11,"rows_kept":75,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,10],[3,7,4,7],[3,8,4,9],[5,3,5,4],[5,8,5,9],[6,3,6,4],[6,8,6,9],[7,3,7,4],[7,8,7,9],[8,3,8,4],[8,8,8,9],[9,3,9,4],[9,8,9,9],[10,0,10,7],[10,8,10,9],[11,0,11,10],[12,0,12,3],[12,4,12,8],[12,9,12,10],[13,0,13,10],[14,0,14,3],[14,4,14,8],[14,9,14,10],[15,0,17,0],[15,1,17,1],[15,2,17,2],[15,3,17,4],[15,5,17,5],[15,6,17,6],[15,7,15,10],[16,7,17,7],[16,8,17,9],[18,3,18,4],[18,8,18,9],[19,3,19,4],[19,8,19,9],[20,3,20,4],[20,8,20,9],[21,0,21,7],[21,8,21,9],[22,0,22,10],[23,0,23,3],[23,4,23,8],[23,9,23,10],[24,0,24,10],[25,0,25,3],[25,4,25,8],[25,9,25,10],[26,0,28,0],[26,1,28,1],[26,2,28,2],[26,3,28,4],[26,5,28,5],[26,6,28,6],[26,7,26,10],[27,7,28,7],[27,8,28,9],[29,3,29,4],[29,8,29,9],[30,3,30,4],[30,8,30,9],[31,3,31,4],[31,8,31,9],[32,3,32,4],[32,8,32,9],[33,0,33,7],[33,8,33,9],[34,0,34,10],[35,0,35,3],[35,4,35,8],[35,9,35,10],[36,0,36,10],[37,0,37,3],[37,4,37,8],[37,9,37,10],[38,0,40,0],[38,1,40,1],[38,2,40,2],[38,3,40,4],[38,5,40,5],[38,6,40,6],[38,7,38,10],[39,7,40,7],[39,8,40,9],[41,3,41,4],[41,8,41,9],[42,3,42,4],[42,8,42,9],[43,3,43,4],[43,8,43,9],[44,3,44,4],[44,8,44,9],[45,3,45,4],[45,8,45,9],[46,3,46,4],[46,8,46,9],[47,0,47,7],[47,8,47,9],[48,0,48,10],[49,0,49,3],[49,4,49,8],[49,9,49,10],[50,0,50,10],[51,0,51,3],[51,4,51,8],[51,9,51,10],[52,0,54,0],[52,1,54,1],[52,2,54,2],[52,3,54,4],[52,5,54,5],[52,6,54,6],[52,7,52,10],[53,7,54,7],[53,8,54,9],[55,3,55,4],[55,8,55,9],[56,3,56,4],[56,8,56,9],[57,3,57,4],[57,8,57,9],[58,3,58,4],[58,8,58,9],[59,3,59,4],[59,8,59,9],[60,3,60,4],[60,8,60,9],[61,3,61,4],[61,8,61,9],[62,3,62,4],[62,8,62,9],[63,3,63,4],[63,8,63,9],[64,3,64,4],[64,8,64,9],[65,3,65,4],[65,8,65,9],[66,3,66,4],[66,8,66,9],[67,3,67,4],[67,8,67,9],[68,3,68,4],[68,8,68,9],[69,3,69,4],[69,8,69,9],[70,3,70,4],[70,8,70,9],[71,0,71,7],[71,8,71,9],[72,0,72,7],[72,8,72,9],[73,0,73,10],[74,0,74,3],[74,4,74,8],[74,9,74,10]]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：园林绿化",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 1 页 共 5 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"整个项目"]
[1,"050101010001","整理绿化用地","1.绿化用地整理\n2.地形微塑造\n3.其他说明:满足图纸规范及相关设计要求",null,"m2","1610"]
[2,"050102001001","栽植乔木","1.种类:香樟树\n2.胸径:15cm\n3.株高、冠径:树高4.5m，冠幅3.5m，分枝点在2m以上，保留3-5主分支,全冠栽植\n4.支撑方式:满足图纸设计要求\n5.草绳缠绕树干\n6.养护期:1年\n7.其他说明:满足图纸规范及相关设计要求",null,"株","9"]
[3,"050102001002","栽植乔木","1.种类:榉树\n2.胸径:15cm\n3.株高、冠径:树高5.5~6m，冠幅3.5~4.5m，分枝点在2.2m以上，保留3-5主分支,全冠栽植\n4.支撑方式:满足图纸设计要求\n5.草绳缠绕树干\n6.养护期:1年\n7.其他说明:满足图纸规范及相关设计要求",null,"株","9"]
[4,"050102001003","栽植乔木","1.种类:黄山栾\n2.胸径:15~18cm\n3.株高、冠径:树高5.0~5.5m，冠幅3.0~3.5m，分枝点在2.5m以上，保留3-5主分支,全冠栽植\n4.支撑方式:满足图纸设计要求\n5.草绳缠绕树干\n6.养护期:1年\n7.其他说明:满足图纸规范及相关设计要求",null,"株","28"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：园林绿化",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 2 页 共 5 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[5,"050102001004","栽植乔木","1.种类:桂花\n2.胸径:12cm\n3.株高、冠径:树高3.0~3.5m，冠幅2.5~3.0m,3~4个主分支以上,分支点大于1.5m,全冠栽植\n4.支撑方式:满足图纸设计要求\n5.养护期:1年\n6.其他说明:满足图纸规范及相关设计要求",null,"株","14"]
[6,"050102001005","栽植乔木","1.种类:石楠\n2.地径:8cm\n3.株高、冠径:树高2.4~2.8m，冠幅1.8~2.2m,枝叶繁茂，株型优美，树干笔直,冠型丰满\n4.支撑方式:满足图纸设计要求\n5.养护期:1年\n6.其他说明:满足图纸规范及相关设计要求",null,"株","4"]
[7,"050102001006","栽植灌木","1.种类:西府海棠\n2.地径:13cm\n3.株高、冠径:树高2.8~3.2m，冠幅2.5~2.8m,冠大,树形饱满,枝干自然,3个主分枝以上,分枝点≥1.2m,全冠种植\n4.支撑方式:满足图纸设计要求\n5.养护期:1年\n6.其他说明:满足图纸规范及相关设计要求",null,"株","11"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：园林绿化",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 3 页 共 5 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[8,"050102001007","栽植灌木","1.种类:日本晚樱\n2.地径:13cm\n3.株高、冠径:树高2.8~3.2m，冠幅2.5~2.8m,冠大,树形饱满,枝干自然,3个主分枝以上,分枝点≥1.2m,全冠种植\n4.支撑方式:满足图纸设计要求\n5.养护期:1年\n6.其他说明:满足图纸规范及相关设计要求",null,"株","7"]
[9,"050102002001","栽植灌木","1.种类:紫荆\n2.株高、冠径:树高2.0~2.2m，冠幅1.8m,丛生,5-6分枝,株型优美,全冠栽植\n3.支撑方式:满足图纸设计要求\n4.养护期:1年\n5.其他说明:满足图纸规范及相关设计要求",null,"株","5"]
[10,"050102002002","栽植灌木","1.种类:海桐球A\n2.株高、冠径:树高1.5m，冠幅1.5m,修剪后蓬径,球形完整\n3.养护期:1年\n4.其他说明:满足图纸规范及相关设计要求",null,"株","12"]
[11,"050102002003","栽植灌木","1.种类:海桐球\n2.株高、冠径:树高1.2m，冠幅1.2m,修剪后蓬径,球形完整\n3.养护期:1年\n4.其他说明:满足图纸规范及相关设计要求",null,"株","32"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：园林绿化",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 4 页 共 5 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[12,"050102007001","栽植色带","1.种类:早园竹\n2.杆径2-3cm,冠幅20cm,高度300cm,营养杯苗,30株/平米,密植满铺\n3.养护期:1年\n4.其他说明:满足图纸规范及相关设计要求",null,"m2","37"]
[13,"050102007002","栽植色带","1.种类:毛杜鹃\n2.冠幅20cm,高度30-35cm,营养杯苗,49株/平米,密植满铺不漏土\n3.养护期:1年\n4.其他说明:满足图纸规范及相关设计要求",null,"m2","63"]
[14,"050102007003","栽植色带","1.种类:葱兰\n2.冠幅20cm,高度25-30cm,64株/平方米,密植满铺\n3.养护期:1年\n4.其他说明:满足图纸规范及相关设计要求",null,"m2","9"]
[15,"050102007004","栽植色带","1.种类:狼尾草\n2.冠幅40-50cm,高度30-40cm,36株/平方米,密植满铺\n3.养护期:1年\n4.其他说明:满足图纸规范及相关设计要求",null,"m2","49"]
[16,"050102007005","栽植色带","1.种类:红花酢浆草\n2.冠径15-20cm,高15-20cm,64株/平方米,盆苗,密植满铺不漏土\n3.养护期:1年\n4.其他说明:满足图纸规范及相关设计要求",null,"m2","65"]
[17,"050102012001","铺种草皮","1.种类:四季青\n2.成品草皮\n3.其他说明:满足图纸规范及相关设计要求",null,"m2","1387"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：园林绿化",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 5 页 共 5 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[18,"050301005001","散布景石","1.自然青石为主,约3块每组,0.2-0.4立方米/块,3-5吨/立方米,因景石布置较多,数量以实际施工为准\n2.其他说明:满足图纸规范及相关设计要求",null,"组","5"]
[19,"050102009001","栽植水生植物","1.种类:睡莲\n2.盆植,多年生,4盆/平方米,1-2头/盆\n3.其他说明:满足图纸规范及相关设计要求",null,"m2","121"]
[20,"050102007006","种植浮岛","1.种类:黄菖蒲\n2.养护期:1年\n3.其他说明:满足图纸规范及相关设计要求",null,"m2","26"]
[21,"050102007007","种植浮岛","1.种类:水生美人蕉\n2.养护期:1年\n3.其他说明:满足图纸规范及相关设计要求",null,"m2","13"]
[null,null,"措施项目"]
{"$rows_empty":11}
["本页小计"]
["合  计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]

{"sheet":"表-11 总价措施项目清单与计价汇总表【园林绿化】","index":13,"n_rows":22,"n_cols":11,"rows_kept":22,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,7],[1,8,1,10],[2,3,2,4],[2,7,2,8],[3,3,3,4],[3,7,3,8],[4,3,4,4],[4,7,4,8],[5,3,5,4],[5,7,5,8],[6,3,6,4],[6,7,6,8],[7,3,7,4],[7,7,7,8],[8,3,8,4],[8,7,8,8],[9,3,9,4],[9,7,9,8],[10,3,10,4],[10,7,10,8],[11,3,11,4],[11,7,11,8],[12,3,12,4],[12,7,12,8],[13,3,13,4],[13,7,13,8],[14,3,14,4],[14,7,14,8],[15,3,15,4],[15,7,15,8],[16,3,16,4],[16,7,16,8],[17,3,17,4],[17,7,17,8],[18,0,18,5],[18,7,18,8],[19,0,19,3],[19,4,19,7],[19,8,19,10],[20,0,20,10],[21,0,21,3],[21,4,21,7],[21,8,21,10]]}
["总价措施项目清单与计价表"]
["工程名称：园林绿化",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":3},"第 1 页 共 1 页"]
["序号","项目编码","项 目 名 称","计 算 基 础",null,"费率(%)","金 额(元)","调整费\n率(%)",null,"调整后金额\n(元)","备 注"]
["1","050405001001","安全文明施工费",{"$nulls":7},"不可竞争费，安全生产费、文明施工措施费费率值根据“豫建设标【2014】57号文”取定，扬尘污染防治费费率值根据“豫建设标【2016】47号文”取定。"]
["1.1","1.1","安全生产费","(综合工日合计+技术措施项目综合工日合计)*34*1.66*(1-10.08%)"]
["1.2","1.2","文明施工措施费","(综合工日合计+技术措施项目综合工日合计)*34*1.66*(1-10.08%)"]
["1.3","1.3","扬尘污染防治费","(综合工日合计+技术措施项目综合工日合计)*34*1.66*(1-10.08%)"]
["2","050405002001","夜间施工增加费","综合工日合计+技术措施项目综合工日合计"]
["3","050405004001","二次搬运费","综合工日合计+技术措施项目综合工日合计"]
["4","050405005001","冬雨季施工增加费","综合工日合计+技术措施项目综合工日合计"]
["5","050405006001","反季节栽植影响措施","综合工日合计+技术措施项目综合工日合计"]
["6","050405007001","地上、地下设施的临时保护设施","综合工日合计+技术措施项目综合工日合计"]
["7","050405008001","已完工程及设备保护费","综合工日合计+技术措施项目综合工日合计"]
[]
[]
[]
[]
[]
["合  计"]
["编制人（造价人员）：",{"$nulls":3},"复核人（造价工程师）："]
["注：1.“计算基础”中安全文明施工费可为“定额基价”、“定额人工费”或“定额人工费+定额机械费”，其他项目可为“定额人工费”或“定额人工费+定额机械费”。\n    2.按施工方案计算的措施费，若无“计算基础”和“费率”的数值，也可只填“金额”数值，但应在备注栏说明施工方案出处或计算方法。"]
[{"$nulls":8},"表-11"]

{"sheet":"表-13 规费、税金项目计价表【园林绿化】","index":14,"n_rows":36,"n_cols":8,"rows_kept":36,"merged":[[0,0,0,7],[1,0,1,2],[1,3,1,5],[1,6,1,7],[2,2,2,3],[2,5,2,6],[3,2,3,3],[3,5,3,6],[4,2,4,3],[4,5,4,6],[5,2,5,3],[5,5,5,6],[6,2,6,3],[6,5,6,6],[7,2,7,3],[7,5,7,6],[8,2,8,3],[8,5,8,6],[9,2,9,3],[9,5,9,6],[10,2,10,3],[10,5,10,6],[11,2,11,3],[11,5,11,6],[12,2,12,3],[12,5,12,6],[13,2,13,3],[13,5,13,6],[14,2,14,3],[14,5,14,6],[15,2,15,3],[15,5,15,6],[16,2,16,3],[16,5,16,6],[17,2,17,3],[17,5,17,6],[18,2,18,3],[18,5,18,6],[19,2,19,3],[19,5,19,6],[20,2,20,3],[20,5,20,6],[21,2,21,3],[21,5,21,6],[22,2,22,3],[22,5,22,6],[23,2,23,3],[23,5,23,6],[24,2,24,3],[24,5,24,6],[25,2,25,3],[25,5,25,6],[26,2,26,3],[26,5,26,6],[27,2,27,3],[27,5,27,6],[28,2,28,3],[28,5,28,6],[29,2,29,3],[29,5,29,6],[30,2,30,3],[30,5,30,6],[31,2,31,3],[31,5,31,6],[32,2,32,3],[32,5,32,6],[33,0,33,4],[33,5,33,6],[34,0,34,2],[34,3,34,7],[35,0,35,2],[35,3,35,5],[35,6,35,7]]}
["规费、税金项目计价表"]
["工程名称：园林绿化",null,null,"标段：襄城县塔湾坑水生态治理及应急排涝项目",null,null,"第 1 页 共 1 页"]
["序号","项 目 名 称","计 算 基 础",null,"计算基数","计算费率\n(%)",null,"金 额(元)"]
["1","规费","其中：1)工程排污费+2)社会保障费+3)住房公积金+4)工伤保险"]
["1.1","其中：1)工程排污费"]
["1.2","2)社会保障费","综合工日合计+技术措施项目综合工日合计"]
["1.3","3)住房公积金","综合工日合计+技术措施项目综合工日合计"]
["1.4","4)工伤保险","综合工日合计+技术措施项目综合工日合计"]
["2","增值税~销项税额","不含税工程造价合计"]
{"$rows_empty":24}
["合  计"]
[" 编制人（造价人员）：",null,null,"复核人（造价工程师）："]
[{"$nulls":6},"表—13"]

{"sheet":"表-14 主要材料价格表【园林绿化】","index":15,"n_rows":18,"n_cols":10,"rows_kept":18,"merged":[[0,0,0,9],[1,0,1,1],[1,2,1,7],[1,8,1,9],[2,1,2,2],[2,7,2,8],[3,1,3,2],[3,7,3,8],[4,1,4,2],[4,7,4,8],[5,1,5,2],[5,7,5,8],[6,1,6,2],[6,7,6,8],[7,1,7,2],[7,7,7,8],[8,1,8,2],[8,7,8,8],[9,1,9,2],[9,7,9,8],[10,1,10,2],[10,7,10,8],[11,1,11,2],[11,7,11,8],[12,1,12,2],[12,7,12,8],[13,1,13,2],[13,7,13,8],[14,1,14,2],[14,7,14,8],[15,1,15,2],[15,7,15,8],[16,1,16,2],[16,7,16,8],[17,1,17,2],[17,7,17,8],[18,1,18,2],[18,7,18,8],[19,1,19,2],[19,7,19,8],[20,1,20,2],[20,7,20,8],[21,1,21,2],[21,7,21,8],[22,1,22,2],[22,7,22,8],[23,1,23,2],[23,7,23,8],[24,1,24,2],[24,7,24,8],[25,1,25,2],[25,7,25,8],[26,1,26,2],[26,7,26,8],[27,1,27,2],[27,7,27,8],[28,1,28,2],[28,7,28,8],[29,1,29,2],[29,7,29,8],[30,1,30,2],[30,7,30,8],[31,1,31,2],[31,7,31,8],[32,1,32,2],[32,7,32,8],[33,1,33,2],[33,7,33,8],[34,1,34,2],[34,7,34,8]]}
["主要材料价格表"]
["工程名称：",null,"园林绿化",{"$nulls":5},"第 1 页 共 1 页"]
["序号","材料编码",null,"材料名称","规格、型号\n等特殊要求","单位","数 量","单 价",null,"合 价"]
[1,"E00008@2",null,"早园竹","高度300cm；30株/平方","m2"]
[2,"E00008@5",null,"狼尾草","狼尾草；冠幅40-50cm；高度30-40cm；36株/平米","m2"]
[3,"E00009@1",null,"毛杜鹃","高度30-35cm；49株/平米","m2"]
[4,"E00010@2",null,"红花酢浆草","冠径15-20cm；高15-20cm；64株/平米","m2"]
[5,"EZ147@1",null,"海桐球A","冠幅150cm","株"]
[6,"EZ147@2",null,"海桐球","冠幅120cm","株"]
[7,"EZ147@3",null,"西府海棠","地径13cm","株"]
[8,"EZ147@4",null,"日本晚樱","地径13cm","株"]
[9,"EZ148@1",null,"桂花","胸径12cm","株"]
[10,"EZ149@1",null,"香樟树","胸径15cm","株"]
[11,"EZ149@2",null,"榉树","胸径15cm","株"]
[12,"EZ149@3",null,"黄山栾","胸径15cm-18cm","株"]
[13,"EZ154@1",null,"石楠","地径8cm","株"]
[14,"EZ1612@1",null,"四季青","成品草坪","m2"]
[15,"EZ635@1",null,"睡莲","4盆/平方米","株"]

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表【电气工程】","index":16,"n_rows":80,"n_cols":11,"rows_kept":80,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,10],[3,7,4,7],[3,8,4,9],[5,3,5,4],[5,8,5,9],[6,3,6,4],[6,8,6,9],[7,3,7,4],[7,8,7,9],[8,3,8,4],[8,8,8,9],[9,3,9,4],[9,8,9,9],[10,3,10,4],[10,8,10,9],[11,3,11,4],[11,8,11,9],[12,3,12,4],[12,8,12,9],[13,3,13,4],[13,8,13,9],[14,0,14,7],[14,8,14,9],[15,0,15,10],[16,0,16,3],[16,4,16,8],[16,9,16,10],[17,0,17,10],[18,0,18,3],[18,4,18,8],[18,9,18,10],[19,0,21,0],[19,1,21,1],[19,2,21,2],[19,3,21,4],[19,5,21,5],[19,6,21,6],[19,7,19,10],[20,7,21,7],[20,8,21,9],[22,3,22,4],[22,8,22,9],[23,3,23,4],[23,8,23,9],[24,3,24,4],[24,8,24,9],[25,3,25,4],[25,8,25,9],[26,3,26,4],[26,8,26,9],[27,3,27,4],[27,8,27,9],[28,3,28,4],[28,8,28,9],[29,3,29,4],[29,8,29,9],[30,3,30,4],[30,8,30,9],[31,0,31,7],[31,8,31,9],[32,0,32,10],[33,0,33,3],[33,4,33,8],[33,9,33,10],[34,0,34,10],[35,0,35,3],[35,4,35,8],[35,9,35,10],[36,0,38,0],[36,1,38,1],[36,2,38,2],[36,3,38,4],[36,5,38,5],[36,6,38,6],[36,7,36,10],[37,7,38,7],[37,8,38,9],[39,3,39,4],[39,8,39,9],[40,3,40,4],[40,8,40,9],[41,3,41,4],[41,8,41,9],[42,3,42,4],[42,8,42,9],[43,3,43,4],[43,8,43,9],[44,3,44,4],[44,8,44,9],[45,3,45,4],[45,8,45,9],[46,0,46,7],[46,8,46,9],[47,0,47,10],[48,0,48,3],[48,4,48,8],[48,9,48,10],[49,0,49,10],[50,0,50,3],[50,4,50,8],[50,9,50,10],[51,0,53,0],[51,1,53,1],[51,2,53,2],[51,3,53,4],[51,5,53,5],[51,6,53,6],[51,7,51,10],[52,7,53,7],[52,8,53,9],[54,3,54,4],[54,8,54,9],[55,3,55,4],[55,8,55,9],[56,3,56,4],[56,8,56,9],[57,3,57,4],[57,8,57,9],[58,3,58,4],[58,8,58,9],[59,3,59,4],[59,8,59,9],[60,3,60,4],[60,8,60,9],[61,3,61,4],[61,8,61,9],[62,3,62,4],[62,8,62,9],[63,3,63,4],[63,8,63,9],[64,3,64,4],[64,8,64,9],[65,3,65,4],[65,8,65,9],[66,3,66,4],[66,8,66,9],[67,3,67,4],[67,8,67,9],[68,3,68,4],[68,8,68,9],[69,3,69,4],[69,8,69,9],[70,3,70,4],[70,8,70,9],[71,3,71,4],[71,8,71,9],[72,3,72,4],[72,8,72,9],[73,3,73,4],[73,8,73,9],[74,3,74,4],[74,8,74,9],[75,3,75,4],[75,8,75,9],[76,0,76,7],[76,8,76,9],[77,0,77,7],[77,8,77,9],[78,0,78,10],[79,0,79,3],[79,4,79,8],[79,9,79,10]]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：电气工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 1 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"整个项目"]
[1,"030404017001","配电箱","1.名称:AL照明配电箱\n2.规格: 600*500*300\n3.安装方式:落地安装\n4.其他详见图纸及规范",null,"台","1"]
[2,"030404017002","配电箱","1.名称:AP动力配电箱\n2.规格: 600*500*300\n3.安装方式:落地安装\n4.其他详见图纸及规范",null,"台","1"]
[3,"030411001001","配管","1.名称:配管\n2.规格:SC25\n3..其他详见图纸及规范",null,"m","20"]
[4,"030411001002","配管","1.名称:配管\n2.规格:SC32\n3..其他详见图纸及规范",null,"m","741.89"]
[5,"030411001003","配管","1.名称:配管\n2.规格:SC40\n3..其他详见图纸及规范",null,"m","95.99"]
[6,"030411001004","配管","1.名称:配管\n2.规格:SC65\n3..其他详见图纸及规范",null,"m","5.87"]
[7,"030411001005","配管","1.名称:配管\n2.规格:SC80\n3..其他详见图纸及规范",null,"m","212"]
[8,"030411001006","配管","1.名称:配管MPP\n2.规格:DN80\n3..其他详见图纸及规范",null,"m","160.54"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：电气工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 2 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[9,"030411004001","配线","1.名称:配线\n2.规格:YJV22-3x6                                                       3.敷设方式：暗敷\n4.其他详见图纸及规范",null,"m","744.89"]
[10,"030411004002","配线","1.名称:配线\n2.规格:YJV22-3X35+2X16\n3.敷设方式：暗敷\n4.其他详见图纸及规范",null,"m","25.25"]
[11,"030411004003","配线","1.名称:配线\n2.规格:YJV22-5X6   \n3.敷设方式：暗敷\n4.其他详见图纸及规范",null,"m","63.72"]
[12,"030411004004","配线","1.名称:配线\n2.规格:YJV22-5X16   \n3.敷设方式：暗敷\n4.其他详见图纸及规范",null,"m","127.8"]
[13,"030412001001","普通灯具","1.名称:照树灯\n2.其他详见图纸及规范",null,"套","42"]
[14,"030412001002","普通灯具","1.名称:庭院灯（含基础）\n2.其他详见图纸及规范",null,"套","23"]
[15,"010404001001","垫层","1.名称:配电箱垫层\n2.规格:石粉垫层\n3.其他详见图纸及规范",null,"m3","0.01"]
[16,"031001006001","塑料管","1.名称:PVC管\n2.规格:50\n3.其他详见图纸及规范",null,"m","29.9"]
[17,"010516001001","螺栓","1.名称:地脚螺栓\n2.规格:M50\n3.其他详见图纸及规范",null,"个","92"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：电气工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 3 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[18,"010516001002","螺栓","1.名称:螺栓\n2.规格:M6\n3.其他详见图纸及规范",null,"个","8"]
[19,"010516002001","预埋铁件","1.名称:角钢\n2.规格:L50*5*2.5\n3.其他详见图纸及规范",null,"根","23"]
[20,"010501001003","垫层","1.混凝土种类:现浇混凝土\n2.混凝土强度等级:C20\n3.其它说明:其他未尽事宜详见施工图设计、现行标准及规范,并满足使用功能要求",null,"m3","0.19"]
[21,"010501003002","独立基础","1.混凝土种类:预拌混凝土\n2.混凝土强度等级:C30\n3.其它说明:其他未尽事宜详见施工图设计、现行标准及规范,并满足使用功能要求",null,"m3","3.68"]
[22,"010515001010","现浇构件钢筋","1.钢筋种类、规格:Φ10以内\n2.其它说明:其他未尽事宜详见施工图设计、现行标准及规范,并满足使用功能要求",null,"t","0.063"]
[23,"031003011001","法兰","1.名称:法兰盲板\n2.厚度:6mm\n3.其它说明:其他未尽事宜详见施工图设计、现行标准及规范,并满足使用功能要求",null,"片","23"]
[24,"010516001003","螺栓","1.名称:螺栓\n2.规格:M20\n3.其它说明:其他未尽事宜详见施工图设计、现行标准及规范,并满足使用功能要求",null,"t","0.146"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：电气工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 4 页 共 4 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[25,"010101003001","挖沟槽土方","1.土壤类别:一二类土\n2.挖土深度:0.9m\n3.其它说明:其他未尽事宜详见施工图设计、现行标准及规范,并满足使用功能要求",null,"m3","99.91"]
[26,"010103001004","回填方","1.填方材料品种:一二类土\n2.其它说明:其他未尽事宜详见施工图设计、现行标准及规范,并满足使用功能要求",null,"m3","99.91"]
[null,null,"措施项目"]
{"$rows_empty":19}
["本页小计"]
["合  计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]

{"sheet":"表-11 总价措施项目清单与计价汇总表【电气工程】","index":17,"n_rows":34,"n_cols":11,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,7],[1,8,1,10],[2,3,2,4],[2,7,2,8],[3,3,3,4],[3,7,3,8],[4,3,4,4],[4,7,4,8],[5,3,5,4],[5,7,5,8],[6,3,6,4],[6,7,6,8],[7,3,7,4],[7,7,7,8],[8,3,8,4],[8,7,8,8],[9,3,9,4],[9,7,9,8],[10,3,10,4],[10,7,10,8],[11,3,11,4],[11,7,11,8],[12,3,12,4],[12,7,12,8],[13,3,13,4],[13,7,13,8],[14,3,14,4],[14,7,14,8],[15,3,15,4],[15,7,15,8],[16,3,16,4],[16,7,16,8],[17,3,17,4],[17,7,17,8],[18,3,18,4],[18,7,18,8],[19,3,19,4],[19,7,19,8],[20,3,20,4],[20,7,20,8],[21,3,21,4],[21,7,21,8],[22,3,22,4],[22,7,22,8],[23,3,23,4],[23,7,23,8],[24,3,24,4],[24,7,24,8],[25,3,25,4],[25,7,25,8],[26,3,26,4],[26,7,26,8],[27,3,27,4],[27,7,27,8],[28,3,28,4],[28,7,28,8],[29,3,29,4],[29,7,29,8],[30,0,30,5],[30,7,30,8],[31,0,31,3],[31,4,31,7],[31,8,31,10],[32,0,32,10],[33,0,33,3],[33,4,33,7],[33,8,33,10]]}
["总价措施项目清单与计价表"]
["工程名称：电气工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":3},"第 1 页 共 1 页"]
["序号","项目编码","项 目 名 称","计 算 基 础",null,"费率(%)","金 额(元)","调整费\n率(%)",null,"调整后金额\n(元)","备 注"]
["1","031302001001","安全文明施工费","分部分项安全文明施工费+单价措施安全文明施工费"]
["2","01","其他措施费（费率类）"]
["2.1","031302002001","夜间施工增加费","分部分项其他措施费+单价措施其他措施费"]
["2.2","031302004001","二次搬运费","分部分项其他措施费+单价措施其他措施费"]
["2.3","031302005001","冬雨季施工增加费","分部分项其他措施费+单价措施其他措施费"]
["3","02","其他（费率类）"]
{"$rows_empty":21}
["合  计"]
["编制人（造价人员）：",{"$nulls":3},"复核人（造价工程师）："]
["注：1.“计算基础”中安全文明施工费可为“定额基价”、“定额人工费”或“定额人工费+定额机械费”，其他项目可为“定额人工费”或“定额人工费+定额机械费”。\n    2.按施工方案计算的措施费，若无“计算基础”和“费率”的数值，也可只填“金额”数值，但应在备注栏说明施工方案出处或计算方法。"]
[{"$nulls":8},"表-11"]

{"sheet":"表-13 规费、税金项目计价表【电气工程】","index":18,"n_rows":37,"n_cols":8,"rows_kept":37,"merged":[[0,0,0,7],[1,0,1,2],[1,3,1,5],[1,6,1,7],[2,2,2,3],[2,5,2,6],[3,2,3,3],[3,5,3,6],[4,2,4,3],[4,5,4,6],[5,2,5,3],[5,5,5,6],[6,2,6,3],[6,5,6,6],[7,2,7,3],[7,5,7,6],[8,2,8,3],[8,5,8,6],[9,2,9,3],[9,5,9,6],[10,2,10,3],[10,5,10,6],[11,2,11,3],[11,5,11,6],[12,2,12,3],[12,5,12,6],[13,2,13,3],[13,5,13,6],[14,2,14,3],[14,5,14,6],[15,2,15,3],[15,5,15,6],[16,2,16,3],[16,5,16,6],[17,2,17,3],[17,5,17,6],[18,2,18,3],[18,5,18,6],[19,2,19,3],[19,5,19,6],[20,2,20,3],[20,5,20,6],[21,2,21,3],[21,5,21,6],[22,2,22,3],[22,5,22,6],[23,2,23,3],[23,5,23,6],[24,2,24,3],[24,5,24,6],[25,2,25,3],[25,5,25,6],[26,2,26,3],[26,5,26,6],[27,2,27,3],[27,5,27,6],[28,2,28,3],[28,5,28,6],[29,2,29,3],[29,5,29,6],[30,2,30,3],[30,5,30,6],[31,2,31,3],[31,5,31,6],[32,2,32,3],[32,5,32,6],[33,2,33,3],[33,5,33,6],[34,0,34,4],[34,5,34,6],[35,0,35,2],[35,3,35,7],[36,0,36,2],[36,3,36,5],[36,6,36,7]]}
["规费、税金项目计价表"]
["工程名称：电气工程",null,null,"标段：襄城县塔湾坑水生态治理及应急排涝项目",null,null,"第 1 页 共 1 页"]
["序号","项 目 名 称","计 算 基 础",null,"计算基数","计算费率\n(%)",null,"金 额(元)"]
["1","规费","定额规费+工程排污费+其他"]
["1.1","定额规费","分部分项规费+单价措施规费"]
["1.2","工程排污费"]
["1.3","其他"]
["2","增值税","不含税工程造价合计"]
{"$rows_empty":26}
["合  计"]
[" 编制人（造价人员）：",null,null,"复核人（造价工程师）："]
[{"$nulls":6},"表—13"]

{"sheet":"表-14 主要材料价格表【电气工程】","index":19,"n_rows":8,"n_cols":10,"rows_kept":8,"merged":[[0,0,0,9],[1,0,1,1],[1,2,1,7],[1,8,1,9],[2,1,2,2],[2,7,2,8],[3,1,3,2],[3,7,3,8],[4,1,4,2],[4,7,4,8],[5,1,5,2],[5,7,5,8],[6,1,6,2],[6,7,6,8],[7,1,7,2],[7,7,7,8],[8,1,8,2],[8,7,8,8],[9,1,9,2],[9,7,9,8],[10,1,10,2],[10,7,10,8],[11,1,11,2],[11,7,11,8],[12,1,12,2],[12,7,12,8],[13,1,13,2],[13,7,13,8],[14,1,14,2],[14,7,14,8],[15,1,15,2],[15,7,15,8],[16,1,16,2],[16,7,16,8],[17,1,17,2],[17,7,17,8],[18,1,18,2],[18,7,18,8],[19,1,19,2],[19,7,19,8],[20,1,20,2],[20,7,20,8],[21,1,21,2],[21,7,21,8],[22,1,22,2],[22,7,22,8],[23,1,23,2],[23,7,23,8],[24,1,24,2],[24,7,24,8],[25,1,25,2],[25,7,25,8],[26,1,26,2],[26,7,26,8],[27,1,27,2],[27,7,27,8],[28,1,28,2],[28,7,28,8],[29,1,29,2],[29,7,29,8],[30,1,30,2],[30,7,30,8],[31,1,31,2],[31,7,31,8],[32,1,32,2],[32,7,32,8],[33,1,33,2],[33,7,33,8],[34,1,34,2],[34,7,34,8],[35,1,35,2],[35,7,35,8],[36,1,36,2],[36,7,36,8]]}
["主要材料价格表"]
["工程名称：",null,"电气工程",{"$nulls":5},"第 1 页 共 1 页"]
["序号","材料编码",null,"材料名称","规格、型号\n等特殊要求","单位","数 量","单 价",null,"合 价"]
[1,"80210561",null,"预拌混凝土","C30","m3"]
[2,"17030103@7",null,"焊接钢管","公称直径DN≤32","m"]
[3,"25000001@3",null,"照树灯","草坪地灯 嵌入式","套"]
[4,"25000001@4",null,"庭院灯","柱灯 ≤3火","套"]
[5,"28031431@7",null,"铜芯绝缘导线","BV-6","m"]

{"sheet":"表-08 分部分项工程和单价措施项目清单与计价表【排水工程】","index":20,"n_rows":144,"n_cols":11,"rows_kept":144,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,10],[3,7,4,7],[3,8,4,9],[5,3,5,4],[5,8,5,9],[6,0,6,7],[6,8,6,9],[7,0,7,10],[8,0,8,3],[8,4,8,8],[8,9,8,10],[9,0,9,10],[10,0,10,3],[10,4,10,8],[10,9,10,10],[11,0,13,0],[11,1,13,1],[11,2,13,2],[11,3,13,4],[11,5,13,5],[11,6,13,6],[11,7,11,10],[12,7,13,7],[12,8,13,9],[14,3,14,4],[14,8,14,9],[15,0,15,7],[15,8,15,9],[16,0,16,10],[17,0,17,3],[17,4,17,8],[17,9,17,10],[18,0,18,10],[19,0,19,3],[19,4,19,8],[19,9,19,10],[20,0,22,0],[20,1,22,1],[20,2,22,2],[20,3,22,4],[20,5,22,5],[20,6,22,6],[20,7,20,10],[21,7,22,7],[21,8,22,9],[23,3,23,4],[23,8,23,9],[24,3,24,4],[24,8,24,9],[25,3,25,4],[25,8,25,9],[26,3,26,4],[26,8,26,9],[27,0,27,7],[27,8,27,9],[28,0,28,10],[29,0,29,3],[29,4,29,8],[29,9,29,10],[30,0,30,10],[31,0,31,3],[31,4,31,8],[31,9,31,10],[32,0,34,0],[32,1,34,1],[32,2,34,2],[32,3,34,4],[32,5,34,5],[32,6,34,6],[32,7,32,10],[33,7,34,7],[33,8,34,9],[35,3,35,4],[35,8,35,9],[36,0,36,7],[36,8,36,9],[37,0,37,10],[38,0,38,3],[38,4,38,8],[38,9,38,10],[39,0,39,10],[40,0,40,3],[40,4,40,8],[40,9,40,10],[41,0,43,0],[41,1,43,1],[41,2,43,2],[41,3,43,4],[41,5,43,5],[41,6,43,6],[41,7,41,10],[42,7,43,7],[42,8,43,9],[44,3,44,4],[44,8,44,9],[45,3,45,4],[45,8,45,9],[46,3,46,4],[46,8,46,9],[47,3,47,4],[47,8,47,9],[48,0,48,7],[48,8,48,9],[49,0,49,10],[50,0,50,3],[50,4,50,8],[50,9,50,10],[51,0,51,10],[52,0,52,3],[52,4,52,8],[52,9,52,10],[53,0,55,0],[53,1,55,1],[53,2,55,2],[53,3,55,4],[53,5,55,5],[53,6,55,6],[53,7,53,10],[54,7,55,7],[54,8,55,9],[56,3,56,4],[56,8,56,9],[57,3,57,4],[57,8,57,9],[58,3,58,4],[58,8,58,9],[59,3,59,4],[59,8,59,9],[60,3,60,4],[60,8,60,9],[61,3,61,4],[61,8,61,9],[62,0,62,7],[62,8,62,9],[63,0,63,10],[64,0,64,3],[64,4,64,8],[64,9,64,10],[65,0,65,10],[66,0,66,3],[66,4,66,8],[66,9,66,10],[67,0,69,0],[67,1,69,1],[67,2,69,2],[67,3,69,4],[67,5,69,5],[67,6,69,6],[67,7,67,10],[68,7,69,7],[68,8,69,9],[70,3,70,4],[70,8,70,9],[71,3,71,4],[71,8,71,9],[72,3,72,4],[72,8,72,9],[73,0,73,7],[73,8,73,9],[74,0,74,10],[75,0,75,3],[75,4,75,8],[75,9,75,10],[76,0,76,10],[77,0,77,3],[77,4,77,8],[77,9,77,10],[78,0,80,0],[78,1,80,1],[78,2,80,2],[78,3,80,4],[78,5,80,5],[78,6,80,6],[78,7,78,10],[79,7,80,7],[79,8,80,9],[81,3,81,4],[81,8,81,9],[82,3,82,4],[82,8,82,9],[83,3,83,4],[83,8,83,9],[84,3,84,4],[84,8,84,9],[85,0,85,7],[85,8,85,9],[86,0,86,10],[87,0,87,3],[87,4,87,8],[87,9,87,10],[88,0,88,10],[89,0,89,3],[89,4,89,8],[89,9,89,10],[90,0,92,0],[90,1,92,1],[90,2,92,2],[90,3,92,4],[90,5,92,5],[90,6,92,6],[90,7,90,10],[91,7,92,7],[91,8,92,9],[93,3,93,4],[93,8,93,9],[94,3,94,4],[94,8,94,9],[95,3,95,4],[95,8,95,9],[96,3,96,4],[96,8,96,9],[97,3,97,4],[97,8,97,9],[98,0,98,7],[98,8,98,9],[99,0,99,10],[100,0,100,3],[100,4,100,8],[100,9,100,10],[101,0,101,10],[102,0,102,3],[102,4,102,8],[102,9,102,10],[103,0,105,0],[103,1,105,1],[103,2,105,2],[103,3,105,4],[103,5,105,5],[103,6,105,6],[103,7,103,10],[104,7,105,7],[104,8,105,9],[106,3,106,4],[106,8,106,9],[107,3,107,4],[107,8,107,9],[108,3,108,4],[108,8,108,9],[109,3,109,4],[109,8,109,9],[110,3,110,4],[110,8,110,9],[111,3,111,4],[111,8,111,9],[112,3,112,4],[112,8,112,9],[113,3,113,4],[113,8,113,9],[114,3,114,4],[114,8,114,9],[115,0,115,7],[115,8,115,9],[116,0,116,10],[117,0,117,3],[117,4,117,8],[117,9,117,10],[118,0,118,10],[119,0,119,3],[119,4,119,8],[119,9,119,10],[120,0,122,0],[120,1,122,1],[120,2,122,2],[120,3,122,4],[120,5,122,5],[120,6,122,6],[120,7,120,10],[121,7,122,7],[121,8,122,9],[123,3,123,4],[123,8,123,9],[124,3,124,4],[124,8,124,9],[125,3,125,4],[125,8,125,9],[126,3,126,4],[126,8,126,9],[127,3,127,4],[127,8,127,9],[128,3,128,4],[128,8,128,9],[129,3,129,4],[129,8,129,9],[130,3,130,4],[130,8,130,9],[131,3,131,4],[131,8,131,9],[132,3,132,4],[132,8,132,9],[133,3,133,4],[133,8,133,9],[134,3,134,4],[134,8,134,9],[135,3,135,4],[135,8,135,9],[136,3,136,4],[136,8,136,9],[137,3,137,4],[137,8,137,9],[138,3,138,4],[138,8,138,9],[139,3,139,4],[139,8,139,9],[140,0,140,7],[140,8,140,9],[141,0,141,7],[141,8,141,9],[142,0,142,10],[143,0,143,3],[143,4,143,8],[143,9,143,10]]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 1 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[null,null,"一体化排涝泵站"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 2 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[1,"030109012001","一体化排涝泵站","1.一体化泵站预制筒体，材质:HMPP，规格:直径3000mm,高度4500mm，HMPP高模量聚丙烯(须提供CMA和CNAS认证机构出具筒体检验报告,弯曲模量不小于1500Mpa),三层缠绕工艺厚度≥65mm\n2.内含铸铁水泵2台，Q=485m3/h,H=10m,N=22kW，二用,一台变频\n3.水泵导轨2套，SUS304，含提升链\n4.水泵自耦底座2套，材质:HT200,规格:DN200\n5.静压液位仪保护管1套，材质:UPVC，规格:DN50，放置静压液位仪,根据液位控制水泵启停\n6.压力管道2套，材质:SUS304，规格:DN250\n7.止回阀2套，材质:HT250，规格:DN250\n8.闸阀2套，材质:HT250，规格:DN250\n9.吊耳1套，材质:Q345，格栅检修时,阻断垃圾进入同时,保证泵站正常运行\n10.出水口软连接1套，材质:可曲挠橡胶，规格:JGD41-10 DN400\n11.进水口软连接1套，材质:可曲挠",null,"台","1"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 3 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[{"$nulls":3},"橡胶，规格:JGD41-10 DN800\n12.提篮格栅1套，材质:SUS304，\n13.格栅导轨1套，材质:SUS304，含提升链\n14.格栅支架1套SUS304，\n15.服务平台1套，GRP格栅板SUS304\n16.扶 梯1套SUS304\n17.盖 板1套压花铝板\n18.安全格栅1套GRP格栅板SUS304\n19.扶手1套SUS304\n20.智能UV离子除臭装置1套组合件风量2000m3/h,设备总功率2.2kW,静音风机\n21.智能控制柜1台不锈钢防水户外型 智能无人值守,状态监控,PLC+触摸屏,软启,远程监控\n22.液位浮球1套PP传感器坏时备用,自动控制水泵启停\n23.90°弯头2套，SUS304，DN250\n24.异径同心大小头2套，SUS304，DN200-250\n25.泵站围栏1套SUS304\n26.其他:详见相关设计图纸及规范要求"]
[2,"070112001001","深水井","1.名称：深水井（水源井）\n2.其他：详见相关设计图纸及规范要求",null,"座","1"]
[null,null,"分部小计"]
[null,null,"一体化污水泵站"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 4 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[1,"030109012002","一体化污水泵站","1.一体化泵站预制筒体，材质:HMPP，规格:直径2000mm,高度4200mm，HMPP高模量聚丙烯(须提供CMA和CNAS认证机构出具筒体检验报告,弯曲模量不小于1500Mpa),三层缠绕工艺厚度≥65mm\n2.内含铸铁水泵2台，Q=30m3/h,H=10m,N=1.5kW，1用1备,一台变频\n3.水泵导轨2套，SUS304，含提升链\n4.水泵自耦底座2套，材质:HT200,规格:DN50\n5.静压液位仪保护管1套，材质:UPVC，规格:DN50，放置静压液位仪,根据液位控制水泵启停\n6.压力管道2套，材质:SUS304，规格:DN65\n7.止回阀2套，材质:HT250，规格:DN65\n8.闸阀2套，材质:HT250，规格:DN65\n9.吊耳1套，材质:Q235，格栅检修时,阻断垃圾进入同时,保证泵站正常运行\n10.出水口软连接1套，材质:可曲挠橡胶，规格:JGD41-10 DN80\n11.进水口软连接1套，材质:可曲挠橡胶，规格:",null,"台","1"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 5 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[{"$nulls":3},"JGD41-10 DN300\n12.粉碎格栅1套，合金钢刀头Q=30m/h,N=1.5kW\n13.格栅导轨1套，材质:SUS304，含提升链\n14.格栅支架1套SUS304，\n15.扶梯1套SUS304\n17.盖板1套压花铝板\n18.安全格栅1套，GRP格栅板SUS304\n19.扶手1套SUS304\n20.智能UV离子除臭装置1套，组合件，风量2000m3/h,设备总功率2.2kW,静音风机\n21.智能控制柜1台，不锈钢防水户外型 智能无人值守,状态监控,PLC+触摸屏,软启,远程监控\n22.液位浮球1套PP，传感器坏时备用,自动控制水泵启停\n23.汇总管1套，SUS304，DN80\n24.异径同心大小头2套，SUS304，DN50~65\n25.泵站围栏1套SUS304\n26.其他:详见相关设计图纸及规范要求"]
[null,null,"分部小计"]
[null,null,"管网铺设"]
[1,"040101002001","挖沟槽土方","1.挖沟槽土方\n2.一、二类土",null,"m3","740"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 6 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[2,"040103001001","回填方","1.回填土\n2.压实度：满足图纸设计及相关规范要求",null,"m3","306"]
[3,"040103001002","回填方","1.管顶以上500mm范围内回填中粗砂\n2.压实度：满足图纸设计及相关规范要求",null,"m3","299"]
[4,"040103002003","余方弃置","1.余方弃置\n2.弃土运距:1KM",null,"m3","434"]
[5,"040103001003","垫层","1.200mm厚中粗砂垫层",null,"m3","96.08"]
[6,"040501004001","塑料管","1.名称：HDPE双壁波纹管\n2.型号：DN300\n3.材质：塑料\n4.连接方式：柔性连接\n5.管道闭水试验 \n6.其他：详见相关设计图纸及规范要求",null,"m","270"]
[7,"040501004002","塑料管","1.名称：HDPE双壁波纹管\n2.型号：DN200\n3.材质：塑料\n4.连接方式：柔性连接                                                5.管道闭水试验 \n6.其他：详见相关设计图纸及规范要求",null,"m","7"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 7 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[8,"040501004003","塑料管","1.名称：HDPE双壁波纹管\n2.型号：DN500\n3.材质：塑料\n4.连接方式：柔性连接                                                    5.管道闭水试验      \n6.其他：详见相关设计图纸及规范要求",null,"m","5"]
[9,"040501004004","塑料管","1.名称：PE80管\n2.型号：DN80\n3.材质：塑料\n4.连接方式：热熔连接                                                      5.管道消毒、冲洗 \n6.其他：详见相关设计图纸及规范要求",null,"m","130"]
[10,"040501004005","塑料管","1.名称：PE80管\n2.型号：DN400\n3.材质：塑料     \n4.连接方式：热熔连接                                                      5.管道消毒、冲洗\n6.其他：详见相关设计图纸及规范要求",null,"m","114"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 8 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[11,"040501004006","塑料管","1.名称：UPVC排水管\n2.型号：De110\n3.材质：塑料\n4.连接方式：柔性连接                                                    5.管道闭水试验       \n6.其他：详见相关设计图纸及规范要求",null,"m","250"]
[12,"040501004007","塑料管","1.名称：UPVC排水管\n2.型号：De150\n3.材质：塑料\n4.连接方式：柔性连接                                                    5.管道闭水试验 \n6.其他：详见相关设计图纸及规范要求",null,"m","9.2"]
[13,"040504001001","砌筑井","1.名称：φ1250砖砌污水消能井\n2.图集：20S515-251\n3.球墨铸铁井盖\n4.井字架\n5.防坠网\n6.其他：详见相关设计图纸及规范要求",null,"座","1"]
[14,"041001009001","破除并恢复井","1.名称：破除并恢复φ1250污水检查井\n2.图集：20S515-30\n3.其他：详见相关设计图纸及规范要求",null,"座","1"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 9 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[15,"040504002001","混凝土井","1.名称：BW1400*1300钢筋混凝土污水进水闸槽井\n2.图集：20S515-317\n3.球墨铸铁井盖\n4.井字架\n5.防坠网\n6.其他：详见相关设计图纸及规范要求",null,"座","1"]
[16,"040504002002","混凝土井","1.名称：φ1000钢筋混凝土雨水检查井\n2.图集：20S515-29\n3.球墨铸铁井盖\n4.井字架\n5.防坠网\n6.其他：详见相关设计图纸及规范要求",null,"座","3"]
[17,"040504003001","塑料检查井","1.名称：污水塑料检查井φ1000\n2.图集：16S524-18\n3.球墨铸铁井盖\n4.井字架\n5.防坠网\n6.其他：详见相关设计图纸及规范要求",null,"座","12"]
[18,"040504002003","混凝土井","1.名称：偏沟式双箅雨水口\n2.图集：16S518-35\n3.球墨铸铁井盖\n4.井字架\n5.防坠网\n6.其他：详见相关设计图纸及规范要求",null,"座","2"]
[19,"040504007001","混凝土出水口","1.名称：八字出水口\n2.图集：20S517-5\n3.其他：详见相关设计图纸及规范要求",null,"座","2"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 10 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[20,"040504001003","砌筑井","1.名称：砖砌雨水消能井\n2.图集：20S515-253\n3.球墨铸铁井盖\n4.井字架\n5.防坠网\n6.其他：详见相关设计图纸及规范要求",null,"座","1"]
[21,"040504001004","破除并恢复井","1.名称：破除并恢复φ1500污水检查井\n2.图集：20S515-29\n3.球墨铸铁井盖\n4.井字架\n5.防坠网\n6.其他：详见相关设计图纸及规范要求",null,"座","1"]
[null,null,"分部小计"]
[null,null,"其他工程"]
[1,"030109012003","坑塘抽水","1.名称：坑塘抽水\n2.其他：详见相关设计图纸及规范要求",null,"m3","4500"]
[2,"040103002004","余方弃置","1.名称：垃圾清运转移\n2.运距：1KM",null,"m3","500"]
[3,"010103002001","淤泥清淤","1.名称：淤泥清淤\n2.运距：1KM",null,"m3","1100"]
[4,"010103002002","盖板沟清淤","1.名称：盖板沟清淤\n2.运距：1KM",null,"m3","220"]
[5,"041001001002","拆除路面","1.破除现状沥青路面\n2.5cm中粒式沥青混凝土、7cm粗粒式沥青混凝土、20cmC20水泥混凝土、20cm级配砂砾石\n3.运距：1KM",null,"m2","28"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":4},"第 11 页 共 11 页"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量","金 额(元)"]
[{"$nulls":7},"综合单价","合 价",null,"其中"]
[{"$nulls":10},"暂估价"]
[6,"040203006002","沥青混凝土","1.5cm 中粒式沥青混凝土(AC-16C)\n2.7cm 粗粒式沥青混凝土(AC-25C)\n3.20cm C20水泥混凝土\n4.20cm 级配砂砾石\n5.其他：详见相关设计图纸及规范要求",null,"m2","28"]
[7,"041001001003","拆除路面","1.破除现状水泥路面\n2.20cm厚C30水泥混凝土、20cm厚级配砂砾石\n3.运距：1KM",null,"m2","610"]
[8,"040203007003","水泥混凝土","1.20cm厚C30水泥混凝土\n2.20cm厚级配砂砾石\n3.路面养护\n4.其他：详见相关设计图纸及规范要求",null,"m2","610"]
[null,null,"分部小计"]
[null,null,"措施项目"]
{"$rows_empty":12}
["本页小计"]
["合  计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[{"$nulls":9},"表—08"]

{"sheet":"表-11 总价措施项目清单与计价汇总表【排水工程】","index":21,"n_rows":34,"n_cols":11,"rows_kept":34,"merged":[[0,0,0,10],[1,0,1,3],[1,4,1,7],[1,8,1,10],[2,3,2,4],[2,7,2,8],[3,3,3,4],[3,7,3,8],[4,3,4,4],[4,7,4,8],[5,3,5,4],[5,7,5,8],[6,3,6,4],[6,7,6,8],[7,3,7,4],[7,7,7,8],[8,3,8,4],[8,7,8,8],[9,3,9,4],[9,7,9,8],[10,3,10,4],[10,7,10,8],[11,3,11,4],[11,7,11,8],[12,3,12,4],[12,7,12,8],[13,3,13,4],[13,7,13,8],[14,3,14,4],[14,7,14,8],[15,3,15,4],[15,7,15,8],[16,3,16,4],[16,7,16,8],[17,3,17,4],[17,7,17,8],[18,3,18,4],[18,7,18,8],[19,3,19,4],[19,7,19,8],[20,3,20,4],[20,7,20,8],[21,3,21,4],[21,7,21,8],[22,3,22,4],[22,7,22,8],[23,3,23,4],[23,7,23,8],[24,3,24,4],[24,7,24,8],[25,3,25,4],[25,7,25,8],[26,3,26,4],[26,7,26,8],[27,3,27,4],[27,7,27,8],[28,3,28,4],[28,7,28,8],[29,3,29,4],[29,7,29,8],[30,0,30,5],[30,7,30,8],[31,0,31,3],[31,4,31,7],[31,8,31,10],[32,0,32,10],[33,0,33,3],[33,4,33,7],[33,8,33,10]]}
["总价措施项目清单与计价表"]
["工程名称：排水工程",{"$nulls":3},"标段：襄城县塔湾坑水生态治理及应急排涝项目",{"$nulls":3},"第 1 页 共 1 页"]
["序号","项目编码","项 目 名 称","计 算 基 础",null,"费率(%)","金 额(元)","调整费\n率(%)",null,"调整后金额\n(元)","备 注"]
["1","041109001001","安全文明施工费","分部分项安全文明施工费+单价措施安全文明施工费"]
["2","01","其他措施费（费率类）"]
["2.1","041109002001","夜间施工增加费","分部分项其他措施费+单价措施其他措施费"]
["2.2","041109003001","二次搬运费","分部分项其他措施费+单价措施其他措施费"]
["2.3","041109004001","冬雨季施工增加费","分部分项其他措施费+单价措施其他措施费"]
["3","02","其他（费率类）"]
{"$rows_empty":21}
["合  计"]
["编制人（造价人员）：",{"$nulls":3},"复核人（造价工程师）："]
["注：1.“计算基础”中安全文明施工费可为“定额基价”、“定额人工费”或“定额人工费+定额机械费”，其他项目可为“定额人工费”或“定额人工费+定额机械费”。\n    2.按施工方案计算的措施费，若无“计算基础”和“费率”的数值，也可只填“金额”数值，但应在备注栏说明施工方案出处或计算方法。"]
[{"$nulls":8},"表-11"]

{"sheet":"表-13 规费、税金项目计价表【排水工程】","index":22,"n_rows":37,"n_cols":8,"rows_kept":37,"merged":[[0,0,0,7],[1,0,1,2],[1,3,1,5],[1,6,1,7],[2,2,2,3],[2,5,2,6],[3,2,3,3],[3,5,3,6],[4,2,4,3],[4,5,4,6],[5,2,5,3],[5,5,5,6],[6,2,6,3],[6,5,6,6],[7,2,7,3],[7,5,7,6],[8,2,8,3],[8,5,8,6],[9,2,9,3],[9,5,9,6],[10,2,10,3],[10,5,10,6],[11,2,11,3],[11,5,11,6],[12,2,12,3],[12,5,12,6],[13,2,13,3],[13,5,13,6],[14,2,14,3],[14,5,14,6],[15,2,15,3],[15,5,15,6],[16,2,16,3],[16,5,16,6],[17,2,17,3],[17,5,17,6],[18,2,18,3],[18,5,18,6],[19,2,19,3],[19,5,19,6],[20,2,20,3],[20,5,20,6],[21,2,21,3],[21,5,21,6],[22,2,22,3],[22,5,22,6],[23,2,23,3],[23,5,23,6],[24,2,24,3],[24,5,24,6],[25,2,25,3],[25,5,25,6],[26,2,26,3],[26,5,26,6],[27,2,27,3],[27,5,27,6],[28,2,28,3],[28,5,28,6],[29,2,29,3],[29,5,29,6],[30,2,30,3],[30,5,30,6],[31,2,31,3],[31,5,31,6],[32,2,32,3],[32,5,32,6],[33,2,33,3],[33,5,33,6],[34,0,34,4],[34,5,34,6],[35,0,35,2],[35,3,35,7],[36,0,36,2],[36,3,36,5],[36,6,36,7]]}
["规费、税金项目计价表"]
["工程名称：排水工程",null,null,"标段：襄城县塔湾坑水生态治理及应急排涝项目",null,null,"第 1 页 共 1 页"]
["序号","项 目 名 称","计 算 基 础",null,"计算基数","计算费率\n(%)",null,"金 额(元)"]
["1","规费","定额规费+工程排污费+其他"]
["1.1","定额规费","分部分项规费+单价措施规费"]
["1.2","工程排污费"]
["1.3","其他"]
["2","增值税","不含税工程造价合计"]
{"$rows_empty":26}
["合  计"]
[" 编制人（造价人员）：",null,null,"复核人（造价工程师）："]
[{"$nulls":6},"表—13"]

{"sheet":"表-14 主要材料价格表【排水工程】","index":23,"n_rows":15,"n_cols":10,"rows_kept":15,"merged":[[0,0,0,9],[1,0,1,1],[1,2,1,7],[1,8,1,9],[2,1,2,2],[2,7,2,8],[3,1,3,2],[3,7,3,8],[4,1,4,2],[4,7,4,8],[5,1,5,2],[5,7,5,8],[6,1,6,2],[6,7,6,8],[7,1,7,2],[7,7,7,8],[8,1,8,2],[8,7,8,8],[9,1,9,2],[9,7,9,8],[10,1,10,2],[10,7,10,8],[11,1,11,2],[11,7,11,8],[12,1,12,2],[12,7,12,8],[13,1,13,2],[13,7,13,8],[14,1,14,2],[14,7,14,8],[15,1,15,2],[15,7,15,8],[16,1,16,2],[16,7,16,8],[17,1,17,2],[17,7,17,8],[18,1,18,2],[18,7,18,8],[19,1,19,2],[19,7,19,8],[20,1,20,2],[20,7,20,8],[21,1,21,2],[21,7,21,8],[22,1,22,2],[22,7,22,8],[23,1,23,2],[23,7,23,8],[24,1,24,2],[24,7,24,8],[25,1,25,2],[25,7,25,8],[26,1,26,2],[26,7,26,8],[27,1,27,2],[27,7,27,8],[28,1,28,2],[28,7,28,8],[29,1,29,2],[29,7,29,8],[30,1,30,2],[30,7,30,8],[31,1,31,2],[31,7,31,8],[32,1,32,2],[32,7,32,8],[33,1,33,2],[33,7,33,8],[34,1,34,2],[34,7,34,8],[35,1,35,2],[35,7,35,8]]}
["主要材料价格表"]
["工程名称：",null,"排水工程",{"$nulls":5},"第 1 页 共 1 页"]
["序号","材料编码",null,"材料名称","规格、型号\n等特殊要求","单位","数 量","单 价",null,"合 价"]
[1,"01010131",null,"钢筋","HRB400φ12","kg"]
[2,"04030143",null,"砂子","中粗砂","m3"]
[3,"80250117@1",null,"沥青混凝土 粗粒式","粗粒式沥青混凝土(AC-25C)","m3"]
[4,"BCCLF84",null,"一体化排涝泵站",null,"台"]
[5,"BCCLF85",null,"一体化污水泵站",null,"台"]
[6,"补充材料001@1",null,"沥青混凝土 中粒式","中粒式沥青混凝土(AC-16C)","m3"]
[7,"80210555",null,"预拌混凝土","C15","m3"]
[8,"80210559",null,"预拌混凝土","C25","m3"]
[9,"80210575@1",null,"预拌混凝土路面","C20","m3"]
[10,"17250261@6",null,"UPVC排水管","De110","m"]
[11,"17250261@8",null,"PE80管","DN400","m"]
[12,"17250261@9",null,"UPVC排水管","De150","m"]